Project Name:	Comprehensive resource assessment for forestry
	Project Code:	CRA	Site ID:	0020	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Henry Smolinski	Locality:
	Date Desc.:	19/03/97	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6394783 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	449015  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	6 % 	Aspect:	270 degrees
	Surface Soil Condition 
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mottled-Subnatric Yellow Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 
	Vegetation:
	Surface Coarse 
	Profile 
	A11	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; 50-90%, rounded, Ironstone, coarse fragments; Field pH 6 (pH meter); 
	A12	0.1 - 0.4 m	Brownish yellow (10YR6/6-Moist); ; Loamy sand; Sandy (grains prominent) fabric; 50-90%, fine gravelly, 
	2-6mm, rounded, Ironstone, coarse fragments; Field pH 6.5 (pH meter); 
	B1	0.4 - 0.6 m	Brownish yellow (10YR6/8-Moist); ; Sandy loam; Weak grade of structure, 2-5 mm, Granular; 50-90%, 
	fine gravelly, 2-6mm, Ironstone, coarse fragments; Field pH 7 (pH meter); 
	B2	0.6 - 1.2 m	Brownish yellow (10YR6/8-Moist); , 2.5YR36, 10-20% , Distinct; , 10YR83, 10-20% , Faint; Clay loam; 
	Massive grade of structure; Weak grade of structure, Platy; Many (20 - 50 %), Ferruginous, , ; Field pH 7
	 (pH meter); 
	Morphological Notes
	B2	Bands of Fe
	Observation Notes
	Site Notes
	changed from 464 (yellow sandy earth) to 301 (deep sandy gravel) on 8/11/2000---really it is 703

	Project Name:	Comprehensive resource assessment for forestry
	Project Code:	CRA	Site ID:	0020	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5B	7B	9.3H	3.53	0.31	0.26	0.29J	13.4D
	6H
	0 - 0.1	5B	7B	9.3H	3.53	0.31	0.26	0.29J	13.4D
	6H
	0.1 - 0.4	5.2B	3B	1.04A	0.9	0.1	0.23	2.27D
	6.7H
	0.1 - 0.4	5.2B	3B	1.04A	0.9	0.1	0.23	2.27D
	6.7H
	0.4 - 0.6	5.2B	4B	2.48H	1.99	0.13	0.17	0.07J	4.77D
	6.5H
	0.4 - 0.6	5.2B	4B	2.48H	1.99	0.13	0.17	0.07J	4.77D
	6.5H
	0.6 - 1.2	6B	5B	0.47H	1.28	0.11	0.17	2.03D
	6.3H
	0.6 - 1.2	6B	5B	0.47H	1.28	0.11	0.17	2.03D
	6.3H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	7.06D	120B	0.198E	4.7	4
	0 - 0.1	7.06D	120B	0.198E	4.7	4
	0.1 - 0.4	1.12D	46B	0.03E	5.6	16.2
	0.1 - 0.4	1.12D	46B	0.03E	5.6	16.2
	0.4 - 0.6	1.49D	50B	0.04E	6.5	24.4
	0.4 - 0.6	1.49D	50B	0.04E	6.5	24.4
	0.6 - 1.2	0.28D	42B	0.013E	6.9	44.6
	0.6 - 1.2	0.28D	42B	0.013E	6.9	44.6
	Laboratory Analyses Completed for this profile
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases

	Project Name:	Comprehensive resource assessment for forestry
	Project Code:	CRA	Site ID:	0020	Observation 	1
	Agency Name:	Agriculture Western Australia
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)