Project Name:	Dandaragan land resources survey
	Project Code:	DAN	Site ID:	0839	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Ted (E.A.) Griffin	Locality:
	Date Desc.:	08/05/96	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6656241 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	364412  Datum: AGD84	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plateau
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Summit surface	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Yellow-Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 
	Profile 
	A1	0 - 0.1 m	Brown (10YR5/3-Moist); ; Clayey sand; Single grain grade of structure; Field pH 5.9 (pH meter); Many, 
	very fine (0-1mm) roots; Clear, Smooth change to - 
	A31	0.1 - 0.3 m	Brownish yellow (10YR6/6-Moist); ; Clayey sand; Single grain grade of structure; Very weak consistence;
	 Field pH 5.6 (pH meter); Many, very fine (0-1mm) roots; Gradual, Smooth change to - 
	A32	0.3 - 1.2 m	Brownish yellow (10YR6/8-Moist); ; Loamy fine sand; Single grain grade of structure; Very weak 
	consistence; Field pH 6.5 (pH meter); Few, very fine (0-1mm) roots; Diffuse, Smooth change to - 
	A33	1.2 - 2.1 m	Brownish yellow (10YR6/8-Moist); ; Clayey fine sand; Single grain grade of structure; Very weak 
	consistence; Field pH 6.3 (pH meter); Few, very fine (0-1mm) roots; 
	B21	2.1 - 3.5 m	Brownish yellow (10YR6/8-Moist); ; Sandy loam; 
	B22	3.5 - 3.9 m	; Fine sandy loam; 
	E	3.9 - 4.2 m	; Clayey coarse sand; 10-20%, fine gravelly, 2-6mm, Quartz, coarse fragments; 2-10%, medium gravelly, 
	6-20mm, Ironstone, coarse fragments; Field pH 6.4 (pH meter); 
	Morphological Notes
	A32	Clay content increases with depth
	Observation Notes
	Site Notes
	occasional blotches (10YR82) below 30 cm

	Project Name:	Dandaragan land resources survey
	Project Code:	DAN	Site ID:	0839	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.4B	6B	1.28H	0.27	0.06	0.06	0.02J	1.67D
	6H
	0 - 0.1	5.4B	6B	1.28H	0.27	0.06	0.06	0.02J	1.67D
	6H
	0.1 - 0.3	4.8B	1B	0.44H	0.11	0.03	0.04	0.03J	0.62D
	5.7H
	0.1 - 0.3	4.8B	1B	0.44H	0.11	0.03	0.04	0.03J	0.62D
	5.7H
	0.2 - 0.24
	0.3 - 0.6	5.5B	1B	0.41H	0.14	0.03	0.05	<0.02J	0.63D
	6.3H
	0.3 - 0.6	5.5B	1B	0.41H	0.14	0.03	0.05	<0.02J	0.63D
	6.3H
	0.6 - 0.9
	0.75 - 0.79
	0.9 - 1.2
	1.2 - 1.5	6.1B	2B	0.27H	0.2	0.03	0.06	<0.02J	0.56D
	6.4H
	1.2 - 1.5	6.1B	2B	0.27H	0.2	0.03	0.06	<0.02J	0.56D
	6.4H
	1.4 - 1.44
	1.5 - 1.8
	1.8 - 2.1	6.2B	1B	0.29H	0.2	0.02	0.06	<0.02J	0.57D
	6.5H
	1.8 - 2.1	6.2B	1B	0.29H	0.2	0.02	0.06	<0.02J	0.57D
	6.5H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.61D	82B	0.04E	1.3	2.1
	0 - 0.1	0.61D	82B	0.04E	1.3	2.1
	0.1 - 0.3	0.17D	27B	0.01E	0.9	3.7
	0.1 - 0.3	0.17D	27B	0.01E	0.9	3.7
	0.2 - 0.24	1.51
	0.3 - 0.6	0.19D	23B	0.007E	1.2	6
	0.3 - 0.6	0.19D	23B	0.007E	1.2	6
	0.6 - 0.9
	0.75 - 0.79	1.54
	0.9 - 1.2
	1.2 - 1.5	0.05D	18B	0.004E	1.5	6.1
	1.2 - 1.5	0.05D	18B	0.004E	1.5	6.1
	1.4 - 1.44	1.54
	1.5 - 1.8
	1.8 - 2.1	0.04D	20B	0.004E	1.7	6.1
	1.8 - 2.1	0.04D	20B	0.004E	1.7	6.1
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available

	Project Name:	Dandaragan land resources survey
	Project Code:	DAN	Site ID:	0839	Observation 	1
	Agency Name:	Agriculture Western Australia
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)
	P3A_NR	Bulk density - Not recorded