Project Name:	Dandaragan land resources survey
	Project Code:	DAN	Site ID:	0849	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	B. Purdie	Locality:
	Date Desc.:	16/05/96	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6607454 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	376200  Datum: AGD84	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	90 degrees
	Surface Soil Condition 	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Arenic Bleached-Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 
	Profile 
	Ap	0 - 0.16 m	Dark grey (2.5Y4/1-Moist); ; Sand; Single grain grade of structure; Moist; Field pH 5 (pH meter); Many, 
	fine (1-2mm) roots; Gradual, Wavy change to - 
	A21	0.16 - 0.7 m	Light brownish grey (2.5Y6/2-Moist); ; Sand; Single grain grade of structure; Dry; Field pH 5.6 (pH 
	meter); Common, fine (1-2mm) roots; Diffuse change to - 
	A22	0.7 - 1.35 m	Light grey (2.5Y7/2-Moist); ; Sand; Single grain grade of structure; Dry; Very weak consistence; Field 
	pH 5.5 (pH meter); Few, fine (1-2mm) roots; Gradual, Wavy change to - 
	B2w	1.35 - 2 m	Pale yellow (2.5Y7/3-Moist); Mechanical, 2.5Y72, 2-10% , 5-15mm, Faint; Sand; Single grain grade of 
	structure; Moist; Very weak consistence; Field pH 5.7 (pH meter); 
	C	2 - 3 m	Light grey (2.5Y7/2-Moist); ; Sand; 
	Morphological Notes
	A21	Moist to 30 cm         
	Observation Notes
	Site Notes
	Basic Arenic Bleached-Orthic Tenosol

	Project Name:	Dandaragan land resources survey
	Project Code:	DAN	Site ID:	0849	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.16	4.5B	2B	0.82H	0.1	0.04	0.05	0.04J	1.01D
	5.4H
	0 - 0.16	4.5B	2B	0.82H	0.1	0.04	0.05	0.04J	1.01D
	5.4H
	0.06 - 0.1
	0.16 - 0.7	4.6B	1B	0.14H	<0.02	<0.02	0.07	0.02J	0.23D
	5.2H
	0.16 - 0.7	4.6B	1B	0.14H	<0.02	<0.02	0.07	0.02J	0.23D
	5.2H
	0.25 - 0.29
	0.56 - 0.6
	0.7 - 1.35	4.6B	0B	0.04H	<0.02	<0.02	0.05	0.02J	0.11D
	5.3H
	0.7 - 1.35	4.6B	0B	0.04H	<0.02	<0.02	0.05	0.02J	0.11D
	5.3H
	0.88 - 0.92
	1.35 - 2	4.7B	0B	0.05H	<0.02	<0.02	0.03	0.03J	0.1D
	5.1H
	1.35 - 2	4.7B	0B	0.05H	<0.02	<0.02	0.03	0.03J	0.1D
	5.1H
	1.41 - 1.45
	2 - 3	4.8B	0B	0.07H	<0.02	<0.02	0.04	0.04J	0.13D
	5.4H
	2 - 3	4.8B	0B	0.07H	<0.02	<0.02	0.04	0.04J	0.13D
	5.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.16	0.47D	50B	0.027E	1.5	0.8
	0 - 0.16	0.47D	50B	0.027E	1.5	0.8
	0.06 - 0.1	1.55
	0.16 - 0.7	0.1D	33B	0.005E	1.2	0.5
	0.16 - 0.7	0.1D	33B	0.005E	1.2	0.5
	0.25 - 0.29	1.51
	0.56 - 0.6	1.59
	0.7 - 1.35	0.05D	28B	0.003E	1.1	0.5
	0.7 - 1.35	0.05D	28B	0.003E	1.1	0.5
	0.88 - 0.92	1.54
	1.35 - 2	0.04D	38B	0.003E	1	0.8
	1.35 - 2	0.04D	38B	0.003E	1	0.8
	1.41 - 1.45	1.61
	2 - 3	0.04D	53B	0.002E	0.4	0.5
	2 - 3	0.04D	53B	0.002E	0.4	0.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts

	Project Name:	Dandaragan land resources survey
	Project Code:	DAN	Site ID:	0849	Observation 	1
	Agency Name:	Agriculture Western Australia
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)
	P3A_NR	Bulk density - Not recorded