Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0147	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Tim Overheu	Locality:
	Date Desc.:	12/03/93	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6306000 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	778800  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Plain
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Soft
	Erosion:	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Limited clearing, for example selective logging
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	Ap	0 - 0.1 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy fine sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Water repellent; Field pH 7.7 (pH meter); 
	A21	0.1 - 0.15 m	Yellowish brown (10YR5/4-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 mm), 
	Concretions; Field pH 7.6 (pH meter); 
	B21	0.15 - 0.95 m	Strong brown (7.5YR5/8-Moist); , 0-0% ; Sandy clay loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; Firm consistence; Field pH 7.6 (pH meter); 
	B22	0.95 - 1.6 m	Strong brown (7.5YR4/8-Moist); Mottles, 5YR44, 2-10% , 15-30mm, Prominent; Light clay; Moderate 
	grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence;
	 Field pH 7.8 (pH meter); 
	C	1.6 - 1.8 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Light clay; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moist; Weak consistence; Field pH 7.9 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0147	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.6B	8B	1.69H	0.49	0.36	0.03	0.12J	2.57D
	5.5H
	0.1 - 0.15	4.8B	2B	1.74H	0.58	0.27	0.03	0.08J	2.62D
	5.9H
	0.15 - 0.95	5.7B	8B	2.33A	2.57	0.26	0.46	6J	5.62D	7.67
	6.6H
	0.95 - 1.6	5.7B	12B	1.09H	2.66	0.16	0.71	0.03J	4.62D
	6.1H
	1.6 - 1.8	5.8B	15B	0.84A	3.35	0.3	1.4	6J	5.89D	23.33
	6.5H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.9D	96B	0.055E	3.7	9.5
	0.1 - 0.15	0.62D	38B	0.034E	4	14.4
	0.15 - 0.95	0.6D	32B	0.041E	4.5	27.5
	0.95 - 1.6	0.1D	19B	0.005E	7	20.6
	1.6 - 1.8	0.1D	19B	0.004E	4.2	52.7
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0147	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)