Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0150	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Tim Overheu	Locality:
	Date Desc.:	12/03/93	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6311900 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	777400  Datum: AGD84	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy4.13
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	Ap	0 - 0.1 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains prominent)
	 fabric; Dry; Loose consistence; Water repellent; Field pH 9.1 (pH meter); 
	B21	0.1 - 0.25 m	Very pale brown (10YR7/4-Moist); , 0-0% ; Light clay; Strong grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Moderately moist; Firm consistence; Field pH 10.7 (pH meter); 
	B22	0.25 - 1 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 10YR72, 2-10% , 5-15mm, Prominent; Light clay; Weak 
	grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence;
	 Soil matrix is Highly calcareous; Field pH 11.1 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Grey clay on kieth guests gypsum trial. Dead sheep pit.    

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0150	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.7B	19B	4.76A	3.92	0.54	0.88	7J	10.1D	12.57
	7.5H
	0.1 - 0.25	8.4B	36B	3.97E	8.76	0.79	6.62	20J	20.14D	33.10
	9.5H
	0.25 - 1	8.7B	64B	1.65E	7.24	1	9.1	18J	18.99D	50.56
	10H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.85D	84B	0.055E	3.1	13.3
	0.1 - 0.25	2C	0.27D	23B	0.021E	3.2	36.3
	0.25 - 1	24C	0.14D	17B	0.012E	4.7	46.8
	Laboratory Analyses Completed for this profile
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0150	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)