Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1139	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Tim Overheu	Locality:
	Date Desc.:	29/11/94	Elevation:	No Data
	Map Ref.:	Rainfall:	400
	Northing/Long.:	6238815 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	681778  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	15 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mottled-Mesonatric Brown Sodosol     	Principal Profile Form:	Dy5.82
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	0-2%, medium gravelly, 6-20mm, subangular, Igneous rock (unidentified); 2-10%, , subangular, Igneous rock (unidentified)
	Profile 
	Ap	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Dry; Loose consistence; Water repellent; Field pH 6.2 (pH meter); Abrupt 
	change to - 
	A21	0.1 - 0.22 m	Dark yellowish brown (10YR4/6-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Field pH 6.7 (pH meter); Clear change to - 
	A3	0.22 - 0.3 m	Brownish yellow (10YR6/6-Moist); , 2-10% , 0-5mm, Prominent; Sand; Single grain grade of structure; 
	Sandy (grains prominent) fabric; Dry; Loose consistence; Field pH 7.1 (pH meter); Abrupt change to - 
	B21	0.3 - 0.7 m	Yellowish brown (10YR5/6-Moist); , 5YR58; Medium clay; Strong grade of structure, 2-5 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; Field pH 8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Site located higher in landscape above a minor drainage line. Contour banks constructed nearby. Nearby paddocks have various planted tree
	 species.  

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1139	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.4B	8B	1.7H	0.36	0.34	0.21	0.24J	2.61D
	5.3H
	0.1 - 0.22	4.2B	3B	0.63H	0.2	0.14	0.09	0.2J	1.06D
	5H
	0.22 - 0.3	5B	4B	0.7H	0.66	0.1	0.24	0.06J	1.7D
	6.1H
	0.3 - 0.7	5.9B	18B	2.3A	5.9	0.59	3.2	11.99D
	6.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.33D	170B	0.105E	1.3A	4.4	3.6
	0.1 - 0.22	0.33D	75B	0.026E	1.4A	4.4	4.2
	0.22 - 0.3	0.16D	71B	0.012E	1.5A	6.9	9
	0.3 - 0.7	0.23D	76B	0.028E	0.8A	4.7	61.9
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	17A1	Total Potassium - X-ray fluorescence
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1139	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)