Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1146	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Tim Overheu	Locality:
	Date Desc.:	23/11/94	Elevation:	80 metres
	Map Ref.:	Rainfall:	500
	Northing/Long.:	6208711 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	699089  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Sand plain
	Morph. Type:	No Data	Relief:	2 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Grey Chromosol     	Principal Profile Form:	Dy5.82
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site 	Cultivation. Rainfed
	Vegetation:
	Surface Coarse 	20-50%, medium gravelly, 6-20mm, subrounded, Gravel; No surface coarse fragments
	Profile 
	Ap	0 - 0.16 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Loamy fine sand; Single grain grade of structure; 
	Sandy (grains prominent) fabric; Dry; Loose consistence; Many (20 - 50 %), Ferruginous, Medium (2 -6 
	mm), Concretions; Water repellent; Field pH 7 (pH meter); Clear change to - 
	A21	0.16 - 0.7 m	Very pale brown (10YR7/4-Moist); ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Very weak consistence; Very many (50 - 100 %), Ferruginous, Medium (2 -6 mm), 
	Concretions; Water repellent; Field pH 6.6 (pH meter); Clear change to - 
	B21	0.7 - 1.42 m	Light grey (10YR7/2-Moist); Mottles, 10YR74, 10-20% , 5-15mm, Distinct; Light medium clay; Massive 
	grade of structure; Sandy (grains prominent) fabric; Moderately moist; Very firm consistence; Very many 
	(50 - 100 %), Ferruginous, Medium (2 -6 mm), Concretions; Field pH 7.8 (pH meter); 
	Morphological Notes
	A21	ABUNDANT GRAVEL AND SAND
	B21	GRAVEL WITH DENSE CLAY MATRIX - INDURATED?
	Observation Notes
	Site Notes
	Duplex soil - sand over gravel over clay on a typical level to gently undulating plain. Area at southern most extention of yilgarn block before 
	bremer and hillup coastal sediments.  

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1146	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.16	4.7B	10B	2.6H	0.57	0.14	0.16	0.24J	3.47D
	5.4H
	0.16 - 0.7	5.1B	6B	0.97H	0.54	0.1	0.23	0.13J	1.84D
	5.7H
	0.7 - 1.42	5.9B	11B	0.6H	2.8	0.17	1	0.14J	4.57D
	6.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.16	1.77D	95B	0.129E	0.12A	2.5	3.5
	0.16 - 0.7	0.33D	26B	0.03E	0.12A	4.7	25.7
	0.7 - 1.42	0.12D	22B	0.009E	0.17A	4.7	25.7
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	17A1	Total Potassium - X-ray fluorescence
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1146	Observation 	1
	Agency Name:	Agriculture Western Australia