Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1915	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Henry Smolinski	Locality:
	Date Desc.:	01/01/94	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6243281 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	759978  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Hypercalcic Brown Sodosol     	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 
	Vegetation:
	Surface Coarse 
	Profile 
	Ap	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Loamy sand; Weak grade of structure, ; Sandy (grains prominent)
	 fabric; Dry; Field pH 6 (pH meter); Clear change to - 
	A2	0.1 - 0.15 m	; Sand; Sandy (grains prominent) fabric; Field pH 7 (pH meter); Abrupt change to - 
	B21t	0.15 - 0.25 m	Yellowish brown (10YR5/4-Moist); Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; , Columnar; 
	Field pH 9 (pH meter); Gradual change to - 
	B22t	0.25 - 0.4 m	Light yellowish brown (2.5Y6/4-Moist); ; Light clay; Weak grade of structure, Angular blocky; Smooth-ped 
	fabric; Moist; Field pH 9 (pH meter); Diffuse change to - 
	B23tk	0.4 - 0.8 m	Pale olive (5Y6/3-Moist); ; Light clay; Massive grade of structure; Moist; Many (20 - 50 %), , , ; Field pH 
	9.1 (pH meter); Diffuse change to - 
	B3	0.8 - 1.2 m	Pale olive (5Y6/3-Moist); ; Light clay; Field pH 9 (pH meter); 
	Morphological Notes
	Ap	(10YR 4/2.5, moist);  (10YR 6/2.5, dry);  Loamy medium to coarse sand;  pH 6.0 - 6.5
	A2	Medium to coarse sand, structureless, compact;  abruupt, irregular boundary.
	B21t	10YR 6.5/4, dry));  Organic staining;  medium to coarse SL. to LSCL.;  coarse columnar structure.
	B3	As above, with common dark segregations (1mm dia.), possibly manganese segregations.  Lime 
	content <10%.
	Observation Notes
	Site Notes
	Soil Pit: 5 (north face).  Soil Class: Hardsetting yellow duplex soil (sand over domed clay).  Soil surface: firm to hardsetting (dry).

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1915	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.3
	0.15 - 0.3
	0.3 - 0.4
	0.4 - 0.7
	0.4 - 0.7
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.3
	0.15 - 0.3
	0.3 - 0.4
	0.4 - 0.7
	0.4 - 0.7
	Laboratory Analyses Completed for this profile
	14B1	Electrical conductivity/SE
	14C1	pH/SE
	14D1_C	Bicarbonate/SE and carbonate/SE - potentiometric titration
	14D2_BC	Bicarbonate/SE and carbonate/SE - indicator method
	14E3	Chloride/SE - ICPAES
	14F1	Sulfate/SE - ICPAES
	14H1_CA	Soluble bases/SE (Ca,Mg,K,Na)
	14H1_K	Soluble bases/SE (Ca,Mg,K,Na)
	14H1_MG	Soluble bases/SE (Ca,Mg,K,Na)
	14H1_NA	Soluble bases/SE (Ca,Mg,K,Na)
	2D1	Moisture content - approximate saturation paste