Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0118	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	18/11/91	Elevation:	310 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6267130 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	550960  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	30 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	135 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dg2.41
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse 	20-50%, medium gravelly, 6-20mm, angular, Quartz; No surface coarse fragments
	Profile 
	A2e	0 - 0.25 m	Pale brown (10YR6/3-Moist); , 0-0% ; Loamy coarse sand; Single grain grade of structure; Moderately 
	moist; 2-10%, Quartz, coarse fragments; Very few (0 - 2 %), Ferruginous, Coarse (6 - 20 mm), Nodules;
	 Field pH 6.5 (Raupach); Common, fine (1-2mm) roots; 
	B21t	0.25 - 0.3 m	Very pale brown (10YR7/4-Moist); Mottles, 10YR68, 20-50% , 5-15mm, Distinct; Light medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Field pH 6.5 (Raupach); 
	B22t	0.3 - 0.5 m	Very pale brown (10YR7/4-Moist); Mottles, 10YR68, 20-50% , 5-15mm, Distinct; Light medium clay; 
	Massive grade of structure; Moderately moist; Field pH 6 (Raupach); 
	Morphological Notes
	A2e	F S QZ & M R GCIS         
	B21t	SAMPLED         
	B22t	SAMPLED         
	Observation Notes
	Site Notes
	Road reserve    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0118	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.25 - 0.5	5.6B	6B	0.88H	2.95	0.07	0.39	<0.02J	4.29D
	6.5H
	0.25 - 0.5	5.6B	6B	0.88H	2.95	0.07	0.39	<0.02J	4.29D
	6.5H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.25 - 0.5	40I	4.5	55.5
	0.25 - 0.5	40I	4.5	55.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded