Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0136	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	28/11/91	Elevation:	280 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6272750 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	572000  Datum: AGD84	Drainage:	Rapidly drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Alluvial plain
	Morph. Type:	Crest	Relief:	3 metres
	Elem. Type:	Lunette	Slope Category:	No Data
	Slope:	5 % 	Aspect:	270 degrees
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc2.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Highly disturbed, for example, quarrying, roadworks, mining, landfill, urban
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1e	0 - 0.3 m	Pale brown (10YR6/3-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Dry; Field pH 7 
	(Raupach); Abundant, fine (1-2mm) roots; Sharp change to - 
	A2e	0.3 - 1.3 m	Yellow (10YR7/6-Moist); Mottles, 5YR56, 0-2% , 0-5mm, Distinct; Fine sand; Massive grade of 
	structure; Sandy (grains prominent) fabric; Dry; Field pH 7 (Raupach); Common, coarse (>5mm) roots; 
	Clear change to - 
	B2w	1.3 - 1.7 m	Brownish yellow (10YR6/8-Moist); Mottles, 7.5YR68, 0-2% , 5-15mm, Distinct; Clayey fine sand; Massive
	 grade of structure; Sandy (grains prominent) fabric; Moist; Few (2 - 10 %), Ferruginous, Medium (2 -6 
	mm), Concretions; Field pH 6.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	A1e	PLUS KS
	A2e	MOTTLES AT 120CM. PLUS KS
	B2w	PLUS KS
	Observation Notes
	Site Notes
	Sand pit in lunette

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0136	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.3	5.2B	2B	1H	0.22	0.07	0.03	0.02J	1.32D
	6.1H
	0 - 0.3	5.2B	2B	1H	0.22	0.07	0.03	0.02J	1.32D
	6.1H
	0.3 - 1.3	6B	2B	0.38A	0.11	0.06	0.05	0.6D
	6.6H
	0.3 - 1.3	6B	2B	0.38A	0.11	0.06	0.05	0.6D
	6.6H
	1.3 - 1.7	6B	1B	0.55A	0.38	0.14	0.07	1.14D
	7H
	1.3 - 1.7	6B	1B	0.55A	0.38	0.14	0.07	1.14D
	7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.3	0.31D	11B	1.8	1.1
	0 - 0.3	0.31D	11B	1.8	1.1
	0.3 - 1.3	0.05D	12B	1.5	2.4
	0.3 - 1.3	0.05D	12B	1.5	2.4
	1.3 - 1.7	0.04D	9B	1.1	7.4
	1.3 - 1.7	0.04D	9B	1.1	7.4
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0136	Observation 	1
	Agency Name:	Agriculture Western Australia
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)