Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0138	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	03/12/91	Elevation:	319 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6326810 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	497860  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	40 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	0 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Vertic Eutrophic Brown Chromosol     	Principal Profile Form:	Dy2.22
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; 2-10%, , subangular, Dolerite
	Profile 
	A1	0 - 0.09 m	Dark reddish brown (5YR3/3-Moist); , 0-0% ; Loam; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Rough-ped fabric; Dry; 10-20%, coarse fragments; Field pH 6 (Raupach); Abundant, fine (1-
	2mm) roots; Clear, Smooth change to - 
	A2	0.09 - 0.56 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Sandy clay loam; Massive grade of structure; Rough-ped fabric;
	 Dry; 20-50%, Dolerite, coarse fragments; Field pH 6.5 (Raupach); Many, fine (1-2mm) roots; Smooth 
	change to - 
	B2t	0.56 - 0.89 m	Yellowish brown (10YR5/6-Moist); , 0-0% ; Medium clay; Strong grade of structure, 20-50 mm, 
	Polyhedral; Smooth-ped fabric; Dry; 20-50%, coarse fragments; Field pH 7 (Raupach); Many, fine (1-
	2mm) roots; Abrupt, Smooth change to - 
	C	0.89 - 1 m	Brownish yellow (10YR6/6-Moist); , 0-0% ; Coarse sand; Massive grade of structure; Dry; 50-90%, 
	Quartz, coarse fragments; Field pH 7 (Raupach); 
	Morphological Notes
	A1	F,M S CONTAINS FINE SAND         
	A2	M S DR FINE FELDSPAR         
	B2t	F A FELD.SLICKENSIDES CDK         
	C	F A QZ & M WEATHERED GRAN         
	Observation Notes
	Site Notes
	100% rock (dolerite) outcrop 20m upslope with York gum -colluvium

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0138	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	5B	5B	8.18H	1.47	0.13	0.15	0.11J	9.93D
	5.8H
	0 - 0.09	5B	5B	8.18H	1.47	0.13	0.15	0.11J	9.93D
	5.8H
	0.09 - 0.56	6B	2B	3.32A	2.13	0.06	0.16	5.67D
	7.2H
	0.09 - 0.56	6B	2B	3.32A	2.13	0.06	0.16	5.67D
	7.2H
	0.56 - 0.89	5.7B	6B	9.09A	9.25	0.16	0.7	19.2D
	6.9H
	0.56 - 0.89	5.7B	6B	9.09A	9.25	0.16	0.7	19.2D
	6.9H
	0.89 - 1	5.6B	2B	6.01A	5	0.09	0.65	11.75D
	7H
	0.89 - 1	5.6B	2B	6.01A	5	0.09	0.65	11.75D
	7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	1.88D	140B	0.137E	12.4	15.3
	0 - 0.09	1.88D	140B	0.137E	12.4	15.3
	0.09 - 0.56	0.21D	43B	0.022E	11.9	17.4
	0.09 - 0.56	0.21D	43B	0.022E	11.9	17.4
	0.56 - 0.89	0.13D	17B	0.015E	8.8	49.9
	0.56 - 0.89	0.13D	17B	0.015E	8.8	49.9
	0.89 - 1	0.12D	35B	0.011E	6.5	11.4
	0.89 - 1	0.12D	35B	0.011E	6.5	11.4
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0138	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)