Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0149	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	10/03/93	Elevation:	350 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6250810 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	493700  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	40 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	5 % 	Aspect:	45 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Yellow Chromosol     	Principal Profile Form:	Dy2.11
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	10-20%, medium gravelly, 6-20mm, subrounded, ; 10-20%, , subrounded, 
	Profile 
	A1	0 - 0.04 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Sandy loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Dry; Firm consistence; 20-50%, medium gravelly, 6-20mm, 
	subrounded, , coarse fragments; 2-10%, coarse gravelly, 20-60mm, subrounded, , coarse fragments; 
	Field pH 6 (Raupach); Common, fine (1-2mm) roots; Abrupt, Smooth change to - 
	B1	0.04 - 0.15 m	Brownish yellow (10YR6/8-Moist); , 0-0% ; Clay loam, sandy; Weak grade of structure, 10-20 mm, 
	Polyhedral; Rough-ped fabric; Dry; Very firm consistence; 20-50%, medium gravelly, 6-20mm, 
	subrounded, , coarse fragments; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Clear, Wavy 
	change to - 
	B2t	0.15 - 0.4 m	Yellow (10YR7/8-Moist); Mottles, 2.5YR48, 2-10% , 5-15mm, Faint; Light medium clay; Weak grade of 
	structure, 20-50 mm, Polyhedral; Rough-ped fabric; Dry; Very firm consistence; 2-10%, fine gravelly, 2-
	6mm, subangular, Granite, coarse fragments; 2-10%, fine gravelly, 2-6mm, subrounded, , coarse 
	fragments; Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 6 (Raupach); 
	Common, fine (1-2mm) roots; Gradual, Wavy change to - 
	C	0.4 - 1.1 m	Yellow (10YR7/8-Moist); , 0-0% ; Sandy light clay; Massive grade of structure; Dry; Weak consistence; 
	10-20%, fine gravelly, 2-6mm, subangular, Granite, coarse fragments; Field pH 6 (Raupach); Few, fine 
	(1-2mm) roots; Abrupt change to - 
	R	1.1 -  m	Rock 
	Morphological Notes
	C	Weathered granite
	R	Granite
	Observation Notes
	Site Notes
	Wattle Creek Catchment soil pit - not described at same time as other pits - granite outcrop 30m downslope.   

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0149	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	5.3B	12B	7.08H	2.07	0.56	0.18	0.1J	9.89D
	6H
	0 - 0.04	5.3B	12B	7.08H	2.07	0.56	0.18	0.1J	9.89D
	6H
	0 - 0.1	5B	14B
	5.7H
	0 - 0.1	5B	14B
	5.7H
	0.04 - 0.15	5.4B	3B	2.98H	1.36	0.41	0.1	0.04J	4.85D
	6.5H
	0.04 - 0.15	5.4B	3B	2.98H	1.36	0.41	0.1	0.04J	4.85D
	6.5H
	0.15 - 0.4	5.7B	4B	1.33H	1.35	0.26	0.11	0.02J	3.05D
	6.5H
	0.15 - 0.4	5.7B	4B	1.33H	1.35	0.26	0.11	0.02J	3.05D
	6.5H
	0.4 - 0.8	5B	3B	0.22H	0.68	0.08	0.04	0.02J	1.02D
	5.4H
	0.4 - 0.8	5B	3B	0.22H	0.68	0.08	0.04	0.02J	1.02D
	5.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	4.93D	210B	0.302E	13.5	15.1
	0 - 0.04	4.93D	210B	0.302E	13.5	15.1
	0 - 0.1	3.58D	160B	0.229E
	0 - 0.1	3.58D	160B	0.229E
	0.04 - 0.15	4.53D	74B	0.09E	11.6	39.2
	0.04 - 0.15	4.53D	74B	0.09E	11.6	39.2
	0.15 - 0.4	0.59D	37B	0.039E	9.9	50.1
	0.15 - 0.4	0.59D	37B	0.039E	9.9	50.1
	0.4 - 0.8	0.08D	20B	0.009E	5.3	22.1
	0.4 - 0.8	0.08D	20B	0.009E	5.3	22.1
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0149	Observation 	1
	Agency Name:	Agriculture Western Australia
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)