Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0152	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	26/03/92	Elevation:	310 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6250730 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	486030  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	40 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	8 % 	Aspect:	90 degrees
	Surface Soil Condition 	Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Magnesic-Natric Red Kurosol     	Principal Profile Form:	Dr2.11
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site 	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse 	2-10%, medium gravelly, 6-20mm, subangular, Ironstone; No surface coarse fragments
	Profile 
	A1	0 - 0.05 m	Dark brown (7.5YR3/2-Moist); , 0-0% ; Clayey fine sand; Massive grade of structure; Dry; 10-20%, fine 
	gravelly, 2-6mm, angular, Quartz, coarse fragments; Strongly water repellent, "Field pH 5 (Raupach); 
	Abundant, fine (1-2mm) roots; Abrupt, Smooth change to - 
	B1	0.05 - 0.15 m	Red (2.5YR4/6-Moist); , 0-0% ; Light clay; Weak grade of structure, 20-50 mm, Polyhedral; Rough-ped 
	fabric; Dry; 50-90%, medium gravelly, 6-20mm, subrounded, , coarse fragments; Many (20 - 50 %), 
	Ferromanganiferous, Coarse (6 - 20 mm), Nodules; Field pH 5 (Raupach); Common, very fine (0-1mm) 
	roots; Clear, Smooth change to - 
	B2	0.15 - 0.7 m	Red (2.5YR4/8-Moist); , 0-0% ; Light medium clay; Strong grade of structure, 20-50 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Field pH 4.5 (Raupach); Few, fine (1-2mm) roots; Gradual, Irregular change to -
	 
	C	0.7 - 1.6 m	White (5YR8/1-Moist); ; Coarse sandy clay loam; Weak grade of structure, Polyhedral; Smooth-ped 
	fabric; Dry; Field pH 4.5 (Raupach); Common, coarse (>5mm) roots; 
	Morphological Notes
	A1	Also fine round smoothfaced ironstone gravel
	C	Kaolinitic clay 30% 30% 10%
	Observation Notes
	Site Notes
	Surface covered with thin (<5mm) veneer of sand

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0152	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.7B	51B
	6.3H
	5.7B
	6.3H
	0 - 0.1	5.7B	51B
	6.3H
	5.7B
	6.3H
	0 - 0.1	5.7B	51B
	6.3H
	5.7B
	6.3H
	0 - 0.1	5.7B	51B
	6.3H
	5.7B
	6.3H
	0.05 - 0.15	4.7B	110B	1.5H	5.82	0.3	1.13	0.89J	8.75D
	5H
	0.05 - 0.15	4.7B	110B	1.5H	5.82	0.3	1.13	0.89J	8.75D
	5H
	0.15 - 0.7	4B	110B	0.25H	5.08	0.11	0.78	1.89J	6.22D
	4.2H
	0.15 - 0.7	4B	110B	0.25H	5.08	0.11	0.78	1.89J	6.22D
	4.2H
	0.7 - 1.6	3.8B	420B	0.05H	4.18	<0.02	1.81	0.95J	6.05D
	3.8H
	0.7 - 1.6	3.8B	420B	0.05H	4.18	<0.02	1.81	0.95J	6.05D
	3.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	10.76D	770B	0.626E
	10.76D	770B	0.626E
	0 - 0.1	10.76D	770B	0.626E
	10.76D	770B	0.626E
	0 - 0.1	10.76D	770B	0.626E
	10.76D	770B	0.626E
	0 - 0.1	10.76D	770B	0.626E
	10.76D	770B	0.626E
	0.05 - 0.15	2.4D	83B	0.071E	13.6	33.1
	0.05 - 0.15	2.4D	83B	0.071E	13.6	33.1
	0.15 - 0.7	0.56D	28B	0.021E	11	59.3
	0.15 - 0.7	0.56D	28B	0.021E	11	59.3
	0.7 - 1.6	0.33D	27B	0.007E	20.6	27.9
	0.7 - 1.6	0.33D	27B	0.007E	20.6	27.9
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0152	Observation 	1
	Agency Name:	Agriculture Western Australia
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)