Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0201	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	14/05/92	Elevation:	245 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6286630 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	510850  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A11	0 - 0.05 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Moist; Very weak 
	consistence; Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Sharp, Smooth change to - 
	A12	0.05 - 0.15 m	Greyish brown (10YR5/2-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Moderately moist; 
	Very weak consistence; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Abrupt, Smooth 
	change to - 
	A2e	0.15 - 0.4 m	Pale brown (10YR6/3-Moist); , 0-0% ; Sand; Single grain grade of structure; Moderately moist; Loose 
	consistence; Field pH 6 (Raupach); Abrupt change to - 
	B21	0.4 - 0.65 m	Light brownish grey (2.5Y6/3-Moist); Mottles, 10YR58, 20-50% , 15-30mm, Prominent; Medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Firm consistence; Field pH 7 
	(Raupach); Clear change to - 
	B22	0.65 -  m	Light brownish grey (2.5Y6/2-Moist); Mottles, 10R46, 20-50% , 5-15mm, Distinct; Medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Firm consistence; Field pH 5 
	(Raupach); 
	Morphological Notes
	B21	Sampled for ESP         
	Observation Notes
	Site Notes
	L1 and L2 have massive structure - made worse by cultivation    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0201	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.63B
	0.16 - 0.26	4.51B
	0.4 - 0.65	6B	48B
	6.5H
	0.4 - 0.65	6B	48B
	6.5H
	0.41 - 0.51	5.6B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.4 - 0.65	56I	6	38
	0.4 - 0.65	56I	6	38
	0.41 - 0.51
	Laboratory Analyses Completed for this profile
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded