Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0353	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Jaki Hogstrom	Locality:
	Date Desc.:	27/07/92	Elevation:	370 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6256720 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	552170  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	50 metres
	Elem. Type:	Summit surface	Slope Category:	No Data
	Slope:	4 % 	Aspect:	0 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	20-50%, medium gravelly, 6-20mm, angular, Quartz; 2-10%, , angular, Quartz
	Profile 
	A1	0 - 0.12 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Moist; 20-50%, 
	medium gravelly, 6-20mm, angular, Quartz, coarse fragments; Field pH 5.5 (Raupach); Many, fine (1-
	2mm) roots; Abrupt change to - 
	A2e	0.12 - 0.25 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Moist; 10-
	20%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; Field pH 5.5 (Raupach); Common, 
	fine (1-2mm) roots; Abrupt, Smooth change to - 
	B21t	0.25 - 0.45 m	Pale brown (10YR6/3-Moist); Mottles, 5YR78, 10-20% , 0-5mm, Distinct; Medium clay; Moderate grade 
	of structure; Rough-ped fabric; Moderately moist; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse 
	fragments; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	B22t	0.45 - 0.5 m	Light grey (10YR7/1-Moist); Mottles, 2.5YR46, 20-50% , 5-15mm, Prominent; Medium clay; Moderate 
	grade of structure; Rough-ped fabric; Moderately moist; Field pH 5.5 (Raupach); Few, very fine (0-1mm) 
	roots; Clear change to - 
	B3	0.5 - 0.7 m	Light grey (10YR7/1-Moist); Mottles, 2.5YR44, 20-50% , 5-15mm, Prominent; Medium clay; Weak grade 
	of structure; Rough-ped fabric; Moderately moist; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse 
	fragments; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Gradual change to - 
	C	0.7 - 0.8 m	White (10YR8/1-Moist); Mottles, 2.5YR44, 20-50% , 5-15mm, Prominent; Light medium clay; Massive 
	grade of structure; Dry; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Field pH 5.5 
	(Raupach); 
	Morphological Notes
	B21t	Very little kaolinite
	B22t	With coarse sand grains. very little kaolinite
	B3	With coarse sand and very fine quartz. Kaolinitic
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0353	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.63B
	0.16 - 0.26	4.39B
	0.25 - 0.45	4.3B	7B	0.39H	1.7	0.09	0.41	0.57J	2.59D
	5.4H
	0.25 - 0.45	4.3B	7B	0.39H	1.7	0.09	0.41	0.57J	2.59D
	5.4H
	0.36 - 0.46	4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.25 - 0.45
	0.25 - 0.45
	0.36 - 0.46
	Laboratory Analyses Completed for this profile
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)