Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0435	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	08/09/92	Elevation:	277 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6280520 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	561750  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	1 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Firm
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	2-10%, medium gravelly, 6-20mm, subrounded, ; No surface coarse fragments
	Profile 
	A1	0 - 0.05 m	Dark brown (10YR3/3-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Abrupt change to - 
	A2e	0.05 - 0.25 m	Pale brown (10YR6/3-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Abrupt change to - 
	B21t	0.25 - 0.6 m	Brownish yellow (10YR6/8-Moist); Mottles, 10YR61, 20-50% , 15-30mm, Prominent; Medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Firm consistence; Field pH 6.5 
	(Raupach); Common, very fine (0-1mm) roots; Clear change to - 
	B22t	0.6 - 1 m	Brownish yellow (10YR6/6-Moist); Mottles, 10YR68, 2-10% , 0-5mm, Faint; Medium clay; Weak grade of 
	structure; Rough-ped fabric; Dry; Firm consistence; Field pH 6.5 (Raupach); Few, very fine (0-1mm) 
	roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	McKenzie Road    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0435	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.67B
	0.16 - 0.26	4.74B
	0.25 - 0.6	5.5B	9B	2.64A	4.44	0.06	0.97	8.11D
	6.5H
	0.25 - 0.6	5.5B	9B	2.64A	4.44	0.06	0.97	8.11D
	6.5H
	0.41 - 0.51	5.6B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.25 - 0.6
	0.25 - 0.6
	0.41 - 0.51
	Laboratory Analyses Completed for this profile
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)