Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0442	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	09/09/92	Elevation:	348 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6283900 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	552210  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	60 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	90 degrees
	Surface Soil Condition 	Firm, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.23
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; 2-10%, , subrounded, Gabbro
	Profile 
	A1	0 - 0.08 m	Dark reddish brown (2.5YR3/3-Moist); , 0-0% ; Clay loam, sandy; Strong grade of structure, 5-10 mm, 
	Granular; Moist; Weak consistence; Field pH 6 (Raupach); Abundant, fine (1-2mm) roots; Abrupt change
	 to - 
	A2	0.08 - 0.4 m	Dark red (2.5YR3/6-Moist); , 0-0% ; Clay loam, sandy; Strong grade of structure; Rough-ped fabric; Wet;
	 Firm consistence; 10-20%, medium gravelly, 6-20mm, rounded, , coarse fragments; Field pH 7 
	(Raupach); Many, fine (1-2mm) roots; Abrupt change to - 
	B21	0.4 - 0.5 m	Dark red (2.5YR3/6-Moist); Mottles, 7.5YR68, 2-10% , 15-30mm, Distinct; Medium clay; Strong grade of
	 structure; Rough-ped fabric; Moderately moist; Firm consistence; Field pH 8 (Raupach); Common, fine 
	(1-2mm) roots; Abrupt change to - 
	B22	0.5 - 0.75 m	Dark red (2.5YR3/6-Moist); Mottles, 7.5YR68, 2-10% , 5-15mm, Distinct; Substrate influence, 10YR82, 
	10-20% , 15-30mm, Distinct; Medium clay; Strong grade of structure; Rough-ped fabric; Moderately 
	moist; Very firm consistence; 20-50%, coarse gravelly, 20-60mm, subrounded, Gabbro, coarse 
	fragments; Field pH 8 (Raupach); Few, very fine (0-1mm) roots; Gradual change to - 
	C	0.75 - 1.3 m	Reddish yellow (7.5YR6/8-Moist); Mottles, 2.5YR48, 10-20% , 15-30mm, Distinct; Sandy light clay; 
	Massive grade of structure; Moderately moist; Firm consistence; Field pH 8.5 (Raupach); Few, very fine 
	(0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	Filmer Road    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0442	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.5B	10B	8H	2.47	0.48	0.35	0.02J	11.3D
	6.3H
	0 - 0.08	5.5B	10B	8H	2.47	0.48	0.35	0.02J	11.3D
	6.3H
	0 - 0.11	5.59B
	0.08 - 0.4	6.3B	4B	5.47A	3.93	0.16	0.71	10.27D
	7.8H
	0.08 - 0.4	6.3B	4B	5.47A	3.93	0.16	0.71	10.27D
	7.8H
	0.08 - 0.4	6.3B	4B	5.47A	3.93	0.16	0.71	10.27D
	7.8H
	0.16 - 0.26	5.99B
	0.4 - 0.5	7B	6B	5.63E	7.4	0.1	1.82	16B	14.95D	11.38
	8.5H
	0.4 - 0.5	7B	6B	5.63E	7.4	0.1	1.82	16B	14.95D	11.38
	8.5H
	0.4 - 0.5	7B	6B	5.63E	7.4	0.1	1.82	16B	14.95D	11.38
	8.5H
	0.4 - 0.5	7B	6B	5.63E	7.4	0.1	1.82	16B	14.95D	11.38
	8.5H
	0.41 - 0.51	6.74B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0 - 0.08
	0 - 0.11
	0.08 - 0.4
	0.08 - 0.4
	0.08 - 0.4
	0.16 - 0.26
	0.4 - 0.5	<2C
	0.4 - 0.5	<2C
	0.4 - 0.5	<2C
	0.4 - 0.5	<2C
	0.41 - 0.51
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0442	Observation 	1
	Agency Name:	Agriculture Western Australia
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)