Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0534	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	28/10/92	Elevation:	345 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6308390 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	513160  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	40 metres
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	1 % 	Aspect:	225 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc2.23
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A11	0 - 0.2 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Moderately moist; 
	Very weak consistence; Field pH 6 (Raupach); Abundant, very fine (0-1mm) roots; Abrupt change to - 
	A12	0.2 - 0.5 m	Dark grey (10YR4/1-Moist); , 0-0% ; Coarse sandy clay loam; Massive grade of structure; Moderately 
	moist; Weak consistence; Field pH 6 (Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	A2e	0.5 - 0.65 m	Light grey (10YR7/2-Moist); , 0-0% ; Clayey coarse sand; Single grain grade of structure; Moist; Weak 
	consistence; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Clear change to - 
	B2t	0.65 - 0.75 m	Very pale brown (10YR7/4-Moist); Mottles, 10YR78, 20-50% , 0-5mm, Distinct; , 10YR62, 10-20% , 0-
	5mm, Faint; Medium clay; Moderate grade of structure; Rough-ped fabric; Moderately moist; Firm 
	consistence; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Abrupt change to - 
	B3	0.75 - 0.9 m	Yellow (10YR8/6-Moist); Mottles, 7.5YR78, 20-50% , 5-15mm, Distinct; Coarse sandy clay loam; Single 
	grain grade of structure; Moderately moist; Very weak consistence; Field pH 6 (Raupach); Gradual 
	change to - 
	C	0.9 - 1 m	Yellow (10YR8/6-Moist); Mottles, 7.5YR78, 20-50% , 5-15mm, Distinct; Coarse sandy loam; Single 
	grain grade of structure; Moderately moist; Very weak consistence; Field pH 6 (Raupach); 
	Morphological Notes
	B2t	Kaolinitic clay. Very slight dispersion         
	Observation Notes
	Site Notes
	Warup Road West - 100m downslope of breakaway    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0534	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.2 - 0.5	4.9B	7B
	6.4H
	0.2 - 0.5	4.9B	7B
	6.4H
	0.5 - 0.65	4.9B	7B
	6.3H
	0.5 - 0.65	4.9B	7B
	6.3H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.2 - 0.5	74I	5.5	20.5
	0.2 - 0.5	74I	5.5	20.5
	0.5 - 0.65	79I	4.5	16.5
	0.5 - 0.65	79I	4.5	16.5
	Laboratory Analyses Completed for this profile
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded