Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0752	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Jaki Hogstrom	Locality:
	Date Desc.:	22/04/93	Elevation:	230 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6296290 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	481680  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	1 metres
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.22
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	Ap	0 - 0.1 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Loamy fine sand; Single grain grade of structure; Moist; Very 
	weak consistence; Water repellent; Field pH 6 (Raupach); Abundant, very fine (0-1mm) roots; Abrupt, 
	Wavy change to - 
	A21	0.1 - 0.2 m	Yellowish brown (10YR5/4-Moist); , 0-0% ; Clayey fine sand; Single grain grade of structure; Moist; 
	Loose consistence; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Gradual change to - 
	A22	0.2 - 0.4 m	Olive yellow (2.5Y6/6-Moist); , 0-0% ; Clayey fine sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 7 (Raupach); Common, fine (1-2mm) roots; Clear change to - 
	B1	0.4 - 0.5 m	Yellowish brown (10YR5/6-Moist); Mottles, 7.5YR56, 2-10% , 0-5mm, Faint; Sandy light clay; Weak 
	grade of structure; Rough-ped fabric; Moderately moist; Very weak consistence; Field pH 7 (Raupach); 
	Few, fine (1-2mm) roots; Clear change to - 
	B21	0.5 - 0.7 m	Yellowish brown (10YR5/6-Moist); Mottles, 5YR46, 20-50% , 5-15mm, Distinct; Light medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Weak consistence; Field pH 7 
	(Raupach); Few, fine (1-2mm) roots; 
	B22	0.7 - 0.8 m	Yellowish brown (10YR5/6-Moist); Mottles, 5YR46, 20-50% , 5-15mm, Distinct; Mottles, 2.5Y61, 2-10% ,
	 5-15mm, Distinct; Medium clay; Massive grade of structure; Moderately moist; Weak consistence; Field 
	pH 7 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	B1	Fine sand in medium sandy light clay         
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0752	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9B
	0.1 - 0.2	4.6B
	0.1 - 0.2	4.6B
	0.4 - 0.5	5.7B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.2	8.1	6.2
	0.1 - 0.2	8.1	6.2
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)