Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0757	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Jaki Hogstrom	Locality:
	Date Desc.:	27/04/93	Elevation:	260 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6305270 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	457010  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Low hills
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Loamy sand; Dry; Very weak consistence; Field pH 
	5.5 (Raupach); Abundant, fine (1-2mm) roots; Abrupt, Wavy change to - 
	A2e	0.05 - 0.1 m	Brown (10YR5/3-Moist); , 0-0% ; Clayey sand; Dry; Loose consistence; Field pH 6 (Raupach); Many, fine
	 (1-2mm) roots; Abrupt, Wavy change to - 
	B2	0.1 - 0.55 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 5YR56, 10-20% , 0-5mm, Distinct; Medium heavy clay; 
	Moderate grade of structure, 50-100 mm, Columnar; Rough-ped fabric; Moderately moist; Strong 
	consistence; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Clear change to - 
	C	0.55 - 0.65 m	Greyish brown (2.5Y5/2-Moist); , 0-0% ; Medium clay; Massive grade of structure; Moderately moist; 
	Firm consistence; Field pH 8.5 (Raupach); Common, fine (1-2mm) roots; 
	Morphological Notes
	A2e	Wavy to 15cm         
	B2	Parting to 5 PO         
	Observation Notes
	Site Notes
	Vegetation shrubby - seems typical of broad valleys in this area    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0757	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.6B
	4.6B
	0 - 0.1	4.6B
	4.6B
	0.1 - 0.3	5.2B	7B	4.06A	11.56	0.16	1.62	17.4D
	6.6H
	0.1 - 0.3	5.2B	7B	4.06A	11.56	0.16	1.62	17.4D
	6.6H
	0.15 - 0.25	4.8B
	0.4 - 0.5	6.6B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0 - 0.1
	0.1 - 0.3	47.5I	8.5	44
	0.1 - 0.3	47.5I	8.5	44
	0.15 - 0.25
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded