Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0823	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	25/05/93	Elevation:	322 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6241140 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	537350  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	20 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy4.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	0-2%, medium gravelly, 6-20mm, angular, Quartz; No surface coarse fragments
	Profile 
	Ap	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Moist; 
	Very weak consistence; 20-50%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 2-10%, 
	medium gravelly, 6-20mm, subrounded, , coarse fragments; Field pH 6 (Raupach); Many, very fine (0-
	1mm) roots; Abrupt change to - 
	A2	0.12 - 0.3 m	Brown (10YR5/3-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Moist; Loose 
	consistence; 10-20%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 20-50%, medium 
	gravelly, 6-20mm, subrounded, , coarse fragments; Field pH 6 (Raupach); Common, very fine (0-1mm) 
	roots; Clear change to - 
	B2	0.3 - 0.5 m	Yellowish brown (10YR5/6-Moist); Mottles, 10R46, 2-10% , 0-5mm, Prominent; Sandy light clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Firm consistence; 20-50%, medium 
	gravelly, 6-20mm, subrounded, , coarse fragments; 20-50%, fine gravelly, 2-6mm, subangular, Quartz, 
	coarse fragments; Common (10 - 20 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6 
	(Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	B3	0.5 - 0.65 m	Yellowish brown (10YR5/8-Moist); , 0-0% ; Clay loam, sandy; Massive grade of structure; Moist; Firm 
	consistence; 50-90%, medium gravelly, 6-20mm, subangular, , coarse fragments; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	A2	KS in CMS
	B3	Stopped by gravel
	Observation Notes
	Site Notes
	Birt Road    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0823	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.8B
	0.15 - 0.25	4.4B
	0.3 - 0.5	4.9B	3B	0.81H	1.94	<0.02	0.15	0.05J	2.91D
	5.7H
	0.3 - 0.5	4.9B	3B	0.81H	1.94	<0.02	0.15	0.05J	2.91D
	5.7H
	0.4 - 0.5	5B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.3 - 0.5	52.5I	5	42.5
	0.3 - 0.5	52.5I	5	42.5
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded