Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1576	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	10/02/94	Elevation:	354 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6278440 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	549570  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	35 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	1 % 	Aspect:	90 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol     	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; 2-10%, , subangular, Dolerite
	Profile 
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); , 0-0% ; Sandy clay loam; Massive grade of structure; Dry; Very firm
	 consistence; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Abrupt, Wavy change to - 
	B2t	0.1 - 0.5 m	Dark reddish brown (2.5YR3/4-Moist); , 0-0% ; Medium clay; Strong grade of structure, 50-100 mm, 
	Prismatic; Smooth-ped fabric; Dry; Very strong consistence; Field pH 6.5 (Raupach); Common, very fine 
	(0-1mm) roots; Clear, Wavy change to - 
	B3	0.5 - 0.8 m	Dark reddish brown (2.5YR3/4-Moist); , 0-0% ; Clay loam, coarse sandy; Weak grade of structure, 20-50 
	mm, Prismatic; Smooth-ped fabric; Dry; Strong consistence; Field pH 7 (Raupach); Few, very fine (0-
	1mm) roots; Clear, Wavy change to - 
	C	0.8 - 1.2 m	, 0-0% ; Massive grade of structure; Dry; Abrupt, Wavy change to - 
	R	1.2 - 1.3 m	Rock 
	Morphological Notes
	B2t	Parting to M,SB,5
	B3	Weathered gabbro about 50%
	C	Weathered gabbro (2mm)
	R	Gabbro?
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1576	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.4B	8B	10H	2.9	0.53	0.35	0.02J	13.78D
	6.1H	7B
	5.3B
	6.1H
	5.4B
	0 - 0.1	5.4B	8B	10H	2.9	0.53	0.35	0.02J	13.78D
	6.1H	7B
	5.3B
	6.1H
	5.4B
	0 - 0.1	5.4B	8B	10H	2.9	0.53	0.35	0.02J	13.78D
	6.1H	7B
	5.3B
	6.1H
	5.4B
	0 - 0.1	5.4B	8B	10H	2.9	0.53	0.35	0.02J	13.78D
	6.1H	7B
	5.3B
	6.1H
	5.4B
	0 - 0.1	5.4B	8B	10H	2.9	0.53	0.35	0.02J	13.78D
	6.1H	7B
	5.3B
	6.1H
	5.4B
	0.1 - 0.3	5.8B	5B	15A	6	0.36	0.43	21.79D
	6.7H
	0.1 - 0.3	5.8B	5B	15A	6	0.36	0.43	21.79D
	6.7H
	0.1 - 0.3	5.8B	5B	15A	6	0.36	0.43	21.79D
	6.7H
	0.15 - 0.25	5.8B
	0.3 - 0.5	6.5B	4B	25A	12	0.57	0.48	38.05D
	7.6H
	0.3 - 0.5	6.5B	4B	25A	12	0.57	0.48	38.05D
	7.6H
	0.3 - 0.5	6.5B	4B	25A	12	0.57	0.48	38.05D
	7.6H
	0.4 - 0.5	6.4B
	0.5 - 0.8	6.5B	3B	19A	9.6	0.34	0.38	29.32D
	7.6H
	0.5 - 0.8	6.5B	3B	19A	9.6	0.34	0.38	29.32D
	7.6H
	0.5 - 0.8	6.5B	3B	19A	9.6	0.34	0.38	29.32D
	7.6H
	0.8 - 1.2	6.4B	3B	20A	10	0.25	0.59	30.84D
	7.5H
	0.8 - 1.2	6.4B	3B	20A	10	0.25	0.59	30.84D
	7.5H

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1576	Observation 	1
	Agency Name:	Agriculture Western Australia
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	2.06D	290B	0.176E	20.1	17.2
	1.9D	280B	0.169E
	0 - 0.1	2.06D	290B	0.176E	20.1	17.2
	1.9D	280B	0.169E
	0 - 0.1	2.06D	290B	0.176E	20.1	17.2
	1.9D	280B	0.169E
	0 - 0.1	2.06D	290B	0.176E	20.1	17.2
	1.9D	280B	0.169E
	0 - 0.1	2.06D	290B	0.176E	20.1	17.2
	1.9D	280B	0.169E
	0.1 - 0.3	0.67D	130B	0.08E	12.9	32.5
	0.1 - 0.3	0.67D	130B	0.08E	12.9	32.5
	0.1 - 0.3	0.67D	130B	0.08E	12.9	32.5
	0.15 - 0.25
	0.3 - 0.5	0.52D	79B	0.062E	10.7	55.5
	0.3 - 0.5	0.52D	79B	0.062E	10.7	55.5
	0.3 - 0.5	0.52D	79B	0.062E	10.7	55.5
	0.4 - 0.5
	0.5 - 0.8	0.21D	110B	0.027E	7.4	25.7
	0.5 - 0.8	0.21D	110B	0.027E	7.4	25.7
	0.5 - 0.8	0.21D	110B	0.027E	7.4	25.7
	0.8 - 1.2	0.09D	140B	0.013E	7.4	17.9
	0.8 - 1.2	0.09D	140B	0.013E	7.4	17.9
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)