Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1589	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	16/02/94	Elevation:	301 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6298710 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	581630  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	25 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc4.11
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	10-20%, medium gravelly, 6-20mm, rounded, ; No surface coarse fragments
	Profile 
	A1p	0 - 0.1 m	Brown (10YR5/3-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Dry; Loose consistence; 
	20-50%, fine gravelly, 2-6mm, subrounded, , coarse fragments; 20-50%, medium gravelly, 6-20mm, 
	subrounded, , coarse fragments; Field pH 5.5 (Raupach); Many, very fine (0-1mm) roots; Abrupt, Smooth 
	change to - 
	A2	0.1 - 0.2 m	Yellowish brown (10YR5/4-Moist); , 0-0% ; Single grain grade of structure; Dry; Loose consistence; 20-
	50%, fine gravelly, 2-6mm, subrounded, , coarse fragments; 20-50%, medium gravelly, 6-20mm, 
	subrounded, , coarse fragments; 20-50%, coarse gravelly, 20-60mm, subrounded, , coarse fragments; 
	Field pH 6 (Raupach); Many, very fine (0-1mm) roots; Abrupt, Irregular change to - 
	B1	0.2 - 0.45 m	Yellowish brown (10YR5/8-Moist); Mottles, 2.5YR46, 10-20% , 0-5mm, Distinct; Massive grade of 
	structure; Dry; 20-50%, fine gravelly, 2-6mm, subrounded, , coarse fragments; 20-50%, medium gravelly, 
	6-20mm, subrounded, , coarse fragments; Many (20 - 50 %), Ferruginous, Medium (2 -6 mm), Nodules; 
	Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6.5 (Raupach); Common, very 
	fine (0-1mm) roots; Clear, Wavy change to - 
	B	0.45 - 1 m	Brownish yellow (10YR6/8-Moist); Mottles, 2.5YR46, 20-50% , 5-15mm, Distinct; Coarse sandy loam; 
	Massive grade of structure; Dry; 10-20%, medium gravelly, 6-20mm, subrounded, , coarse fragments; 
	Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6.5 (Raupach); Few, very fine (0-
	1mm) roots; Clear change to - 
	C	1 - 1.5 m	White (10YR8/1-Moist); Mottles, 10R36, 20-50% , 15-30mm, Distinct; Mottles, 10YR66, 10-20% , 5-
	15mm, Distinct; Clay loam; Weak grade of structure, Polyhedral; Smooth-ped fabric; Dry; Field pH 6.5 
	(Raupach); 
	Morphological Notes
	A2	MSL         
	B1	+ CKS - roots in cracks         
	B	Mottled zone         
	Observation Notes
	Site Notes
	Datatine Soil Pit 4    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1589	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.8B	9B	2.5H	0.62	0.71	0.11	0.17J	3.94D
	5.6H	10B
	4.9B
	5.7H
	4.8B
	0 - 0.1	4.8B	9B	2.5H	0.62	0.71	0.11	0.17J	3.94D
	5.6H	10B
	4.9B
	5.7H
	4.8B
	0 - 0.1	4.8B	9B	2.5H	0.62	0.71	0.11	0.17J	3.94D
	5.6H	10B
	4.9B
	5.7H
	4.8B
	0 - 0.1	4.8B	9B	2.5H	0.62	0.71	0.11	0.17J	3.94D
	5.6H	10B
	4.9B
	5.7H
	4.8B
	0 - 0.1	4.8B	9B	2.5H	0.62	0.71	0.11	0.17J	3.94D
	5.6H	10B
	4.9B
	5.7H
	4.8B
	0.1 - 0.2	5.4B	4B	2.2H	0.83	0.26	0.13	<0.02J	3.42D
	6.2H
	5.1B
	0.1 - 0.2	5.4B	4B	2.2H	0.83	0.26	0.13	<0.02J	3.42D
	6.2H
	5.1B
	0.1 - 0.2	5.4B	4B	2.2H	0.83	0.26	0.13	<0.02J	3.42D
	6.2H
	5.1B
	0.2 - 0.45	5.8B	6B	1.9H	1.8	0.16	0.27	<0.02J	4.13D
	6.1H
	0.2 - 0.45	5.8B	6B	1.9H	1.8	0.16	0.27	<0.02J	4.13D
	6.1H
	0.3 - 0.4	5.6B
	0.45 - 0.75	5.6B	20B	1.1H	2.7	0.09	0.78	<0.02J	4.67D
	5.6H
	0.45 - 0.75	5.6B	20B	1.1H	2.7	0.09	0.78	<0.02J	4.67D
	5.6H
	0.45 - 0.75	5.6B	20B	1.1H	2.7	0.09	0.78	<0.02J	4.67D
	5.6H
	0.75 - 1	5.4B	21B	0.75H	2.8	0.04	0.66	<0.02J	4.25D
	5.4H
	0.75 - 1	5.4B	21B	0.75H	2.8	0.04	0.66	<0.02J	4.25D
	5.4H
	0.75 - 1	5.4B	21B	0.75H	2.8	0.04	0.66	<0.02J	4.25D
	5.4H

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1589	Observation 	1
	Agency Name:	Agriculture Western Australia
	1 - 1.5	5.3B	24B	0.5H	3.1	0.03	0.92	<0.02J	4.55D
	5.4H
	1 - 1.5	5.3B	24B	0.5H	3.1	0.03	0.92	<0.02J	4.55D
	5.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.51D	200B	0.113E	5.2	9.7
	1.52D	220B	0.109E
	0 - 0.1	1.51D	200B	0.113E	5.2	9.7
	1.52D	220B	0.109E
	0 - 0.1	1.51D	200B	0.113E	5.2	9.7
	1.52D	220B	0.109E
	0 - 0.1	1.51D	200B	0.113E	5.2	9.7
	1.52D	220B	0.109E
	0 - 0.1	1.51D	200B	0.113E	5.2	9.7
	1.52D	220B	0.109E
	0.1 - 0.2	0.43D	48B	0.031E	4.6	8.3
	0.1 - 0.2	0.43D	48B	0.031E	4.6	8.3
	0.1 - 0.2	0.43D	48B	0.031E	4.6	8.3
	0.2 - 0.45	0.24D	31B	0.02E	7	10.3
	0.2 - 0.45	0.24D	31B	0.02E	7	10.3
	0.3 - 0.4
	0.45 - 0.75	0.1D	23B	0.008E	10.7	18
	0.45 - 0.75	0.1D	23B	0.008E	10.7	18
	0.45 - 0.75	0.1D	23B	0.008E	10.7	18
	0.75 - 1	0.05D	17B	0.004E	13.4	25.8
	0.75 - 1	0.05D	17B	0.004E	13.4	25.8
	0.75 - 1	0.05D	17B	0.004E	13.4	25.8
	1 - 1.5	0.05D	25B	0.005E	14.6	36.2
	1 - 1.5	0.05D	25B	0.005E	14.6	36.2
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)