Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1592	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	17/05/94	Elevation:	230 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6295540 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	492490  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	1 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	No effective disturbance. Natural
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.07 m	Dark grey (10YR4/1-Moist); , 0-0% ; Coarse sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Abrupt change to - 
	A2e	0.07 - 0.3 m	Light brownish grey (10YR6/2-Moist); ; Coarse sand; Massive grade of structure; Dry; Very weak 
	consistence; Field pH 6 (Raupach); Common, very fine (0-1mm) roots; Gradual change to - 
	A3e	0.3 - 0.55 m	Pale brown (10YR6/3-Moist); , 0-0% ; Clayey coarse sand; Massive grade of structure; Dry; Weak 
	consistence; Field pH 5 (Raupach); Common, very fine (0-1mm) roots; Clear change to - 
	B21	0.55 - 0.75 m	Brown (10YR5/3-Moist); Mottles, 7.5YR56, 2-10% , 5-15mm, Distinct; Sandy light clay; Moderate grade 
	of structure, Columnar; Rough-ped fabric; Dry; Field pH 5 (Raupach); Few, very fine (0-1mm) roots; 
	Clear change to - 
	B22	0.75 - 0.9 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR56, 2-10% , 0-5mm, Faint; Sandy light clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Field pH 4.5 (Raupach); Few, very 
	fine (0-1mm) roots; 
	B3	0.9 - 1.25 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 10YR58, 20-50% , 15-30mm, Distinct; Sandy light medium 
	clay; Moderate grade of structure; Rough-ped fabric; Moderately moist; Gradual change to - 
	C	1.25 - 1.5 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 10-20% , 15-30mm, Faint; Light clay; Moderate grade of 
	structure; Rough-ped fabric; Moderately moist; Field pH 6.5 (Raupach); 
	Morphological Notes
	B21	Slight dispersion         
	Observation Notes
	Site Notes
	Site in nature reserve along Bokal East Road.  Moist to 5cm. Saline land about 50m away.

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1592	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.5B	28B
	5.2H
	0.15 - 0.25	4.7B	17B
	5.4H
	0.4 - 0.5	4.4B	42B
	5.1H
	0.55 - 0.75	4.2B	98B	0.88H	0.48	0.06	0.15	0.04J	1.57D
	4.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.4 - 0.5
	0.55 - 0.75	57.5I	10	32.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded