Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1947	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	25/08/94	Elevation:	240 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6265260 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	487210  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	20 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	225 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Brown Chromosol     	Principal Profile Form:	Dy2.22
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	10-20%, medium gravelly, 6-20mm, rounded, ; No surface coarse fragments
	Profile 
	A1	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Moderately 
	moist; 20-50%, fine gravelly, 2-6mm, rounded, , coarse fragments; 2-10%, medium gravelly, 6-20mm, 
	rounded, , coarse fragments; Field pH 6 (Raupach); Abrupt change to - 
	A21	0.12 - 0.3 m	Dark yellowish brown (10YR4/4-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; 10-20%, 
	fine gravelly, 2-6mm, rounded, , coarse fragments; 20-50%, medium gravelly, 6-20mm, rounded, , coarse 
	fragments; Field pH 6.5 (Raupach); Gradual change to - 
	A22	0.3 - 0.55 m	Yellowish brown (10YR5/4-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; 10-20%, fine 
	gravelly, 2-6mm, rounded, , coarse fragments; 20-50%, medium gravelly, 6-20mm, rounded, , coarse 
	fragments; Field pH 7 (Raupach); Clear change to - 
	B2	0.55 - 0.8 m	Yellowish brown (10YR5/8-Moist); , 0-0% ; Sandy light medium clay; Moderate grade of structure; 
	Moderately moist; 10-20%, medium gravelly, 6-20mm, rounded, , coarse fragments; Field pH 7.5 
	(Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1947	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.4B
	0.15 - 0.25	5.8B
	0.4 - 0.5	5.8B
	0.55 - 0.75	6.1B	3B	1.6A	2.1	0.11	0.2	4.01D
	6.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.4 - 0.5
	0.55 - 0.75	64.5I	5.5	30
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded