Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2317	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	12/04/95	Elevation:	280 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6302120 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	512910  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	20 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	270 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mottled-Subnatric Yellow Sodosol     	Principal Profile Form:	Dy3.12
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1p	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Dry; 10-
	20%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Field pH 5.5 (Raupach); Many, very 
	fine (0-1mm) roots; Sharp, Smooth change to - 
	A3e	0.08 - 0.23 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Clayey coarse sand; Massive grade of structure; Dry; 
	20-50%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 10-20%, medium gravelly, 6-
	20mm, subrounded, , coarse fragments; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; 
	Abrupt, Smooth change to - 
	B2	0.23 - 0.55 m	Brownish yellow (10YR6/6-Moist); , 10YR72, 2-10% , 5-15mm, Distinct; , 7.5YR58, 10-20% , 5-15mm, 
	Distinct; Light medium clay; Weak grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric; Dry; 
	Field pH 6 (Raupach); Few, fine (1-2mm) roots; Clear, Wavy change to - 
	C11	0.55 - 1.05 m	Brownish yellow (10YR6/6-Moist); Mottles, 7.5YR58, 2-10% , 15-30mm, Distinct; , 2.5YR46, 2-10% , 5-
	15mm, Distinct; Coarse sandy clay loam; Massive grade of structure; Dry; 20-50%, medium gravelly, 6-
	20mm, angular, Granite, coarse fragments; 10-20%, medium gravelly, 6-20mm, subrounded, , coarse 
	fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6.5 (Raupach); Few, 
	fine (1-2mm) roots; Clear, Smooth change to - 
	C12	1.05 - 1.4 m	White (10YR8/1-Moist); Mottles, 10YR68, 10-20% , 15-30mm, Distinct; , 2.5YR46, 2-10% , 5-15mm, 
	Distinct; Coarse sandy light clay; Massive grade of structure; Dry; 10-20%, medium gravelly, 6-20mm, 
	subrounded, , coarse fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 
	6.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	C11	Weathered granite
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2317	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	4.4B	7B	2H	0.51	0.09	0.15	0.37J	2.75D
	5.3H
	0 - 0.08	4.4B	7B	2H	0.51	0.09	0.15	0.37J	2.75D
	5.3H
	0 - 0.1	4.3B	5B
	5.3H
	0 - 0.1	4.3B	5B
	5.3H
	0.08 - 0.23	4.1B	2B	0.46H	0.29	0.04	0.06	0.41J	0.85D
	5.2H
	0.08 - 0.23	4.1B	2B	0.46H	0.29	0.04	0.06	0.41J	0.85D
	5.2H
	0.23 - 0.43	5.5B	5B	1.4H	2.6	0.03	0.26	<0.02J	4.29D
	6H
	0.23 - 0.43	5.5B	5B	1.4H	2.6	0.03	0.26	<0.02J	4.29D
	6H
	0.43 - 0.55	5.7B	6B	1H	3.6	0.02	0.39	<0.02J	5.01D
	6.2H
	0.43 - 0.55	5.7B	6B	1H	3.6	0.02	0.39	<0.02J	5.01D
	6.2H
	0.55 - 0.85	5.5B	7B	0.4H	2.6	0.02	0.4	<0.02J	3.42D
	5.9H
	0.55 - 0.85	5.5B	7B	0.4H	2.6	0.02	0.4	<0.02J	3.42D
	5.9H
	0.85 - 1.05	5.3B	8B	0.16H	2.8	0.03	0.49	<0.02J	3.48D
	5.8H
	0.85 - 1.05	5.3B	8B	0.16H	2.8	0.03	0.49	<0.02J	3.48D
	5.8H
	1.05 - 1.4	5.4B	8B	0.07H	3.7	0.02	0.62	<0.02J	4.41D
	6.2H
	1.05 - 1.4	5.4B	8B	0.07H	3.7	0.02	0.62	<0.02J	4.41D
	6.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	1.87D	120B	0.136E	6.1	5.8
	0 - 0.08	1.87D	120B	0.136E	6.1	5.8
	0 - 0.1	1.61D	100B	0.121E
	0 - 0.1	1.61D	100B	0.121E
	0.08 - 0.23	0.28D	33B	0.025E	5.4	11.1
	0.08 - 0.23	0.28D	33B	0.025E	5.4	11.1
	0.23 - 0.43	0.16D	42B	0.026E	6.5	42.9
	0.23 - 0.43	0.16D	42B	0.026E	6.5	42.9
	0.43 - 0.55	0.09D	29B	0.016E	6.1	40.2
	0.43 - 0.55	0.09D	29B	0.016E	6.1	40.2
	0.55 - 0.85	0.05D	18B	0.005E	7.5	25.5
	0.55 - 0.85	0.05D	18B	0.005E	7.5	25.5
	0.85 - 1.05	0.03D	18B	0.005E	6.8	27.6
	0.85 - 1.05	0.03D	18B	0.005E	6.8	27.6

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2317	Observation 	1
	Agency Name:	Agriculture Western Australia
	1.05 - 1.4	0.05D	15B	0.005E	7.4	26.7
	1.05 - 1.4	0.05D	15B	0.005E	7.4	26.7
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)