Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2338	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	21/09/95	Elevation:	285 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6315060 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	584930  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.13
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Cultivation. Rainfed
	Vegetation:
	Surface Coarse 	10-20%, medium gravelly, 6-20mm, subrounded, ; No surface coarse fragments
	Profile 
	Ap	0 - 0.1 m	Dark reddish brown (5YR3/2-Moist); , 0-0% ; Clay loam; Massive grade of structure; Dry; Very firm 
	consistence; 10-20%, medium gravelly, 6-20mm, rounded, , coarse fragments; Common (10 - 20 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 7.5 (Raupach); Common, very fine (0-1mm) 
	roots; Abrupt, Smooth change to - 
	B21	0.1 - 0.25 m	Red (2.5YR4/6-Moist); , 0-0% ; Medium clay; Moderate grade of structure, 20-50 mm, Polyhedral; 
	Rough-ped fabric; Dry; Very firm consistence; Common (10 - 20 %), Ferromanganiferous, Medium (2 -6 
	mm), Nodules; Soil matrix is Very highly calcareous; Field pH 9.5 (Raupach); Common, very fine (0-
	1mm) roots; Clear, Wavy change to - 
	B22	0.25 - 0.7 m	Red (2.5YR4/6-Moist); , 0-0% ; Medium heavy clay; Massive grade of structure; Rough-ped fabric; Dry; 
	Strong consistence; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; Many (20 - 
	50 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Soil matrix is Highly calcareous; Field pH 9.5 
	(Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	B23k	0.7 - 1.5 m	Red (2.5YR4/6-Moist); , 0-0% ; Medium clay; Weak grade of structure, 20-50 mm, Polyhedral; Smooth-
	ped fabric; Dry; Strong consistence; Many (20 - 50 %), Calcareous, Extremely coarse (> 60 mm), Soft 
	segregations; Many (20 - 50 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), 
	Calcareous, Coarse (6 - 20 mm), Nodules; Soil matrix is Slightly calcareous; Field pH 9.5 (Raupach); 
	Morphological Notes
	Ap	Black gravel
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2338	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.6B	58B	10.47A	5.02	1.19	0.43	17.11D
	6.8H
	0 - 0.1	6.6B	58B	10.47A	5.02	1.19	0.43	17.11D
	6.8H
	0.1 - 0.25	8.1B	30B	9.99E	9.42	1.3	1.91	20B	22.62D	9.55
	8.8H
	0.1 - 0.25	8.1B	30B	9.99E	9.42	1.3	1.91	20B	22.62D	9.55
	8.8H
	0.25 - 0.55	8.4B	36B	4.89E	10.12	1.7	4.32	20B	21.03D	21.60
	9.5H
	0.25 - 0.55	8.4B	36B	4.89E	10.12	1.7	4.32	20B	21.03D	21.60
	9.5H
	0.55 - 0.7	8.6B	67B	1.61E	8.26	1.88	8.38	20B	20.13D	41.90
	9.8H
	0.55 - 0.7	8.6B	67B	1.61E	8.26	1.88	8.38	20B	20.13D	41.90
	9.8H
	0.7 - 1	8.7B	77B	0.88E	7.5	1.89	10.62	20B	20.89D	53.10
	9.8H
	0.7 - 1	8.7B	77B	0.88E	7.5	1.89	10.62	20B	20.89D	53.10
	9.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0C	1.28D	230B	0.09E	11.3	20
	0 - 0.1	0C	1.28D	230B	0.09E	11.3	20
	0.1 - 0.25	5C	0.48D	93B	0.04E	11.1	44.2
	0.1 - 0.25	5C	0.48D	93B	0.04E	11.1	44.2
	0.25 - 0.55	18C	0.2D	62B	0.022E	8.8	47
	0.25 - 0.55	18C	0.2D	62B	0.022E	8.8	47
	0.55 - 0.7	19C	0.11D	48B	0.014E	9.3	51.3
	0.55 - 0.7	19C	0.11D	48B	0.014E	9.3	51.3
	0.7 - 1	16C	0.08D	41B	0.012E	11	49.7
	0.7 - 1	16C	0.08D	41B	0.012E	11	49.7
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2338	Observation 	1
	Agency Name:	Agriculture Western Australia
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)