Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2352	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Angela Stuart-Street	Locality:
	Date Desc.:	30/10/97	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6273546 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	548311  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Firm, Hardsetting
	Erosion:	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Ferric Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A11	0 - 0.17 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Dry; Firm consistence; 10-20%, medium 
	gravelly, 6-20mm, rounded, Ironstone, coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, 
	Quartz, coarse fragments; 
	A21	0.17 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Loamy coarse sand; Dry; Firm consistence; 20-50%, fine gravelly, 2-
	6mm, rounded, Ironstone, coarse fragments; 10-20%, fine gravelly, 2-6mm, subangular, Quartz, coarse 
	fragments; 
	B21c	0.3 - 0.65 m	Yellowish brown (10YR5/6-Moist); ; Coarse sandy loam; Dry; Firm consistence; 20-50%, fine gravelly, 2-
	6mm, rounded, Ironstone, coarse fragments; 20-50%, medium gravelly, 6-20mm, rounded, Ironstone, 
	coarse fragments; 
	B22	0.65 - 0.8 m	Brownish yellow (10YR6/8-Moist); ; Coarse sandy loam; Dry; Very firm consistence; 10-20%, fine 
	gravelly, 2-6mm, subangular, Quartz, coarse fragments; 2-10%, medium gravelly, 6-20mm, subangular, 
	Granite, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes
	Surface of paddock has moderate cover, many bare patches between pasture. Compaction of surface again, Penetrometer reading  >6kg/cm.
	 Good rooting depth >30cm into A2 horizon; Compaction pan 10 - 15cm. (see "Veg. & Loc. notes" for more.)

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2352	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.6B	4B
	5.8H
	0.7 - 0.8	5.3B	5B
	6.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.22D	0.089E	94.5I	2.5	3
	0.7 - 0.8	0.13D	86.5I	3.5	10
	Laboratory Analyses Completed for this profile
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1e	Nitrate-N, in presence of nitrite
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded