Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0011	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Mir Frahmand	Locality:
	Date Desc.:	03/03/95	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6592650 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	438350  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	135 degrees
	Surface Soil Condition 	Hardsetting
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Mesotrophic Grey Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Sandy loam; , ; Dry; Field pH 6.8 (pH meter); Clear change to - 
	B2t	0.05 - 0.3 m	Greyish brown (10YR5/2-Moist); ; Clay loam; Massive grade of structure; Dry; Field pH 7.5 (pH meter); 
	Diffuse change to - 
	B21t	0.3 - 0.6 m	Greyish brown (10YR5/2-Moist); ; Medium clay; Dry; Field pH 7.8 (pH meter); Diffuse change to - 
	B22tc	0.6 - 0.9 m	Light grey (10YR7/2-Moist); , 5YR46; Medium clay; Massive grade of structure; Dry; 50-90%, angular, 
	Ironstone, coarse fragments; Field pH 6.1 (pH meter); Diffuse change to - 
	B23t	0.9 - 1 m	Very pale brown (10YR7/4-Moist); ; Medium clay; Massive grade of structure; Dry; 
	Morphological Notes
	B2t	Disp
	B21t	Disp
	Observation Notes
	Site Notes
	Surface cracking 2mm wide.  side of pit cracking but sealed on the top.  Column block  Lenticular

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0011	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.5B	24B	5.42H	2.45	0.48	0.34	0.02J	8.69D
	6.1H
	0.05 - 0.3	6B	12B	4.46A	3.4	0.22	0.74	8.82D
	7H
	0.3 - 0.6	5.7B	19B	1.7A	3.65	0.36	1.61	7.32D
	6.8H
	0.6 - 0.9	4.5B	28B	1.09H	3.43	0.43	1.88	0.11J	6.83D
	5.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	2.15D	200B	0.113E	10.4	17.2
	0.05 - 0.3	1.35D	99B	0.053E	8.2	30
	0.3 - 0.6	0.36D	58B	0.025E	8.1	46.2
	0.6 - 0.9	0.29D	65B	0.019E	10.5	53.2
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0011	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)