Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0189	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Mir Frahmand	Locality:
	Date Desc.:	12/08/96	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6707644 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	448441  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Rises
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	135 degrees
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Petroclcic Red Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Clayey coarse sand; , Granular; Field pH 6.6 (pH meter); Clear 
	change to - 
	B1t	0.1 - 0.25 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Moderate grade of structure; Field pH 7.1 (pH meter); Diffuse 
	change to - 
	B2t	0.25 - 0.45 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Moderate grade of structure; Field pH 7.8 (pH meter); 
	Diffuse change to - 
	B22tc	0.45 - 0.7 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Moderate grade of structure; 20-50%, coarse gravelly, 20-
	60mm, subrounded, Calcrete, coarse fragments; Soil matrix is Slightly calcareous; Field pH 8.6 (pH 
	meter); 
	Cm	0.7 -  m	; Calcrete, Moderately cemented, Nodular; Soil matrix is Highly calcareous; Field pH 8.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Fine roots in profile.

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0189	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6B	5B	1.87A	0.6	0.56	0.06	3.09D
	7H
	0.1 - 0.25	6.2B	2B	4.08A	1.28	0.35	0.22	5.93D
	7.6H
	0.25 - 0.45	7.1B	3B	5.33E	1.83	0.22	0.77	10B	8.15D	7.70
	8.8H
	0.45 - 0.7	8.1B	13B	5.9E	2.71	0.23	1.98	12B	10.82D	16.50
	9.3H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.56D	180B	0.046E	5.3	7.4
	0.1 - 0.25	0.24D	4.1	19.4
	0.25 - 0.45	0.16D	4.5	24.6
	0.45 - 0.7	<2C	0.09D	8.8	23.4
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0189	Observation 	1
	Agency Name:	Agriculture Western Australia
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)