Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0503	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Mir Frahmand	Locality:
	Date Desc.:	01/01/95	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6640069 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	472978  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endohypersodic Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (2.5YR3/3-Moist); ; Sandy loam; Moderate grade of structure, ; Field pH 7.6 (pH 
	meter); Clear change to - 
	B21t	0.1 - 0.35 m	Red (2.5YR4/6-Moist); ; Clay loam; Weak grade of structure, Polyhedral; Clear change to - 
	B22tk	0.35 - 0.65 m	Red (2.5YR4/6-Moist); ; Light clay; Moderate grade of structure, Angular blocky; 20-50%, Calcrete, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Soft segregations; Clear change to - 
	B23tk	0.65 - 1 m	Reddish brown (2.5YR4/4-Moist); , 2.5Y21; Light clay; Moderate grade of structure, Angular blocky; 20-
	50%, coarse gravelly, 20-60mm, subrounded, Calcrete, coarse fragments; Common (10 - 20 %), 
	Calcareous, , Soft segregations; Diffuse change to - 
	B24tk	1 - 1.3 m	Red (2.5YR4/8-Moist); ; Sandy light clay; Weak grade of structure, Angular blocky; 0-2%, Calcrete, 
	coarse fragments; Very few (0 - 2 %), Calcareous, , Soft segregations; Field pH 9.6 (pH meter); Diffuse 
	change to - 
	B25tk	1.3 - 1.6 m	Red (2.5YR5/6-Moist); ; Sandy light clay; 
	Morphological Notes
	B23tk	layer of manganoferous covered the K ndules
	Observation Notes
	Site Notes

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0503	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1B	9B	4.63A	2.17	1.23	0.18	8.21D
	6.9H
	0.1 - 0.35	6.4B	4B	8.35A	4.11	1.38	0.26	14.1D
	7.5H
	0.35 - 0.65	8.1B	12B	8.76E	5.06	1.1	0.64	18B	15.56D	3.56
	8.9H
	0.65 - 1	8.3B	24B	4.95E	5.6	1.6	2.37	17B	14.52D	13.94
	9.5H
	1 - 1.3	8.5B	46B	2.38E	5.38	1.9	5.4	16B	15.06D	33.75
	9.8H
	1.3 - 1.6	8.6B	71B	1.43E	5.17	2.02	7.28	16B	15.9D	45.50
	9.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.59D	160B	0.052E	8.2	13.7
	0.1 - 0.35	0.37D	7.5	30.5
	0.35 - 0.65	6C	0.27D	9.5	38
	0.65 - 1	10C	0.12D	8.9	35.8
	1 - 1.3	15C	0.08D	6.9	38.1
	1.3 - 1.6	14C	0.08D	8.9	40.8
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	0503	Observation 	1
	Agency Name:	Agriculture Western Australia
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)