Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0312	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	31/07/95	Elevation:	290 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6243795 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	626780  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	5 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Hypernatric Brown Sodosol     	Principal Profile Form:	Dy2.41
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, angular, Quartz; 2-10%, , subangular, Quartz
	Profile Morphology
	A1	0 - 0.08 m	Very dark brown (10YR2/2-Moist); , 0-0% ; Sand; Massive grade of structure; Moderately moist; Field pH
	 6 (Raupach); Abrupt change to - 
	A2e	0.08 - 0.12 m	Pale brown (10YR6/3-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Moderately moist; Field 
	pH 6 (Raupach); Abrupt, Wavy change to - 
	B2	0.12 - 0.4 m	Strong brown (7.5YR5/8-Moist); , 0-0% ; Medium clay; Moderate grade of structure; Smooth-ped fabric; 
	Dry; Field pH 6 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	Lupins in paddock to north of site - "hardsetting grey clay".

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0312	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	4.6B	13B	1.93H	0.56	0.26	0.11	0.13J	2.86D
	5.7H
	0 - 0.08	4.6B	13B	1.93H	0.56	0.26	0.11	0.13J	2.86D
	5.7H
	0 - 0.08	4.6B	13B	1.93H	0.56	0.26	0.11	0.13J	2.86D
	5.7H
	0.12 - 0.32	4.8B	16B	0.92H	2.82	0.22	1.7	0.24J	5.66D
	6H
	0.12 - 0.32	4.8B	16B	0.92H	2.82	0.22	1.7	0.24J	5.66D
	6H
	0.12 - 0.32	4.8B	16B	0.92H	2.82	0.22	1.7	0.24J	5.66D
	6H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	1.59D	92.5I	3	4.5
	0 - 0.08	1.59D	92.5I	3	4.5
	0 - 0.08	1.59D	92.5I	3	4.5
	0.12 - 0.32	0.56D	40.5I	2.5	57
	0.12 - 0.32	0.56D	40.5I	2.5	57
	0.12 - 0.32	0.56D	40.5I	2.5	57
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded