Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0476	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	19/09/95	Elevation:	340 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6285480 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	622920  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	15 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	45 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Hypernatric Yellow Sodosol     	Principal Profile Form:	Dy2.13
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, subangular, Quartz; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Dry; Field pH 6 
	(Raupach); Abrupt, Wavy change to - 
	B2t	0.1 - 0.3 m	Light brown (7.5YR6/4-Moist); , 0-0% ; Sandy medium clay; Moderate grade of structure; Rough-ped 
	fabric; Dry; Field pH 7.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	Site in remnant mallee along fence line.

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0476	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8B	60B	3.3H	4.72	0.18	0.55	<0.02J	8.75D
	6.3H
	0 - 0.1	5.8B	60B	3.3H	4.72	0.18	0.55	<0.02J	8.75D
	6.3H
	0 - 0.1	5.8B	60B	3.3H	4.72	0.18	0.55	<0.02J	8.75D
	6.3H
	0.1 - 0.3	6.6B	68B	2.85A	7.61	0.14	2.1	12.7D
	7.3H
	0.1 - 0.3	6.6B	68B	2.85A	7.61	0.14	2.1	12.7D
	7.3H
	0.1 - 0.3	6.6B	68B	2.85A	7.61	0.14	2.1	12.7D
	7.3H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.37D	75.5I	4	20.5
	0 - 0.1	1.37D	75.5I	4	20.5
	0 - 0.1	1.37D	75.5I	4	20.5
	0.1 - 0.3	0.88D	54.5I	4	41.5
	0.1 - 0.3	0.88D	54.5I	4	41.5
	0.1 - 0.3	0.88D	54.5I	4	41.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0476	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded