Project Name:	Southern Cross Hyden land resources survey
	Project Code:	SCS	Site ID:	0313	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Mir Frahmand	Locality:
	Date Desc.:	28/10/92	Elevation:	340 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6508514 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	654326  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Peneplain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	315 degrees
	Surface Soil Condition 	Loose
	Erosion	 (wind); 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Fine sandy loam; Single grain grade of structure; Water repellent; Field 
	pH 7.3 (pH meter); 
	0.1 - 0.2 m	Brown (7.5YR4/4-Moist); ; Fine sandy clay loam; Massive grade of structure; 50-90%, subrounded, 
	Calcrete, coarse fragments; 2-10%, medium gravelly, 6-20mm, Ironstone, coarse fragments; Field pH 8 
	(pH meter); 
	0.2 - 0.55 m	Brown (7.5YR4/4-Moist); ; Light clay; Massive grade of structure; 50-90%, subrounded, Calcrete, coarse
	 fragments; 20-50%, subangular, Ironstone, coarse fragments; Field pH 9.1 (pH meter); 
	0.55 - 1.1 m	Light brown (7.5YR6/4-Moist); ; Light clay; Massive grade of structure; 20-50%, medium gravelly, 6-
	20mm, angular, Calcrete, coarse fragments; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), Soft 
	segregations; , Calcareous, , Nodules; Field pH 9.3 (pH meter); 
	Morphological Notes
	         
	PALLID ZONE--CALCAREOUS ROCKS?         
	PALLID ZONE--CALCAREOUS ROCKS?         
	PALLID ZONE--CALCAREOUS ROCKS?         
	Observation Notes
	Site Notes
	Day rd--Catchment group soil pit--Gravelly brown sandy loam/clay    

	Project Name:	Southern Cross Hyden land resources survey
	Project Code:	SCS	Site ID:	0313	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1B	15B	4.41A	2.35	0.45	0.67	6J	7.88D	11.17
	6.7H
	0.1 - 0.2	7.6B	150B	6.47E	7.35	1.31	3.03	18J	18.16D	16.83
	8H
	0.2 - 0.55	8.2B	430B	4.66E	8.74	1.54	3.82	16J	18.76D	23.88
	8.5H
	0.55 - 1.1	8.4B	320B	2.3E	6.24	1.44	6.19	14J	16.17D	44.21
	8.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.39D	74B	0.068E	4.1	11.3
	0.1 - 0.2	<2C	0.84D	33B	0.05E	4.7	43.9
	0.2 - 0.55	23C	0.29D	32B	0.032E	11.2	39.5
	0.55 - 1.1	18C	0.17D	28B	0.015E	13.8	16.9
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)

	Project Name:	Southern Cross Hyden land resources survey
	Project Code:	SCS	Site ID:	0313	Observation 	1
	Agency Name:	Agriculture Western Australia
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)