Project Name:	Southern Cross Hyden land resources survey
	Project Code:	SCS	Site ID:	1121	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Mir Frahmand	Locality:
	Date Desc.:	19/08/94	Elevation:	360 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6395099 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	673965  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	90 degrees
	Surface Soil Condition 	Soft
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Regolithic Yellow-Orthic Tenosol Thick  Loamy  Deep	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data and little or no knowledge of this soil.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	0 - 0.15 m	; Clayey sand; Field pH 5.1 (pH meter); Gradual change to - 
	0.15 - 0.85 m	; Fine sandy loam; Field pH 4.7 (pH meter); Diffuse change to - 
	0.85 - 0.9 m	; Fine sandy loam; 2-10%, fine gravelly, 2-6mm, rounded, Ironstone, coarse fragments; Many (20 - 50 %),
	 , , Soft segregations; Field pH 4.9 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Soil type: WCS/gSL SIS

	Project Name:	Southern Cross Hyden land resources survey
	Project Code:	SCS	Site ID:	1121	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.4B	1B	0.16H	0.08	0.04	<0.02	0.12J	0.29D
	5.1H
	0.15 - 0.85	4B	2B	0.15H	0.11	0.03	0.02	0.06J	0.31D
	4.4H
	0.85 - 0.95	4.2B	2B	0.26H	0.56	0.02	0.04	0.36J	0.88D
	4.6H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	0.16D	16B	0.009E	1.1	5.5
	0.15 - 0.85	0.12D	14B	0.012E	3.5	20.8
	0.85 - 0.95	0.07D	23B	0.009E	3.4	11.6
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)