Project Name:	Sandstone Yalgoo Paynes Find rangeland survey
	Project Code:	SYP	Site ID:	I016	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Mark Newell	Locality:
	Date Desc.:	13/09/92	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6947813 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	720639  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	30 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Cryptogam surface, Hardsetting
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Lithosolic Clastic Rudosol  Non-gravelly Sandy  Shallow	Principal Profile Form:	Uc5.21
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A11	0 - 0.05 m	Yellowish red (5YR4/6-Moist); ; Clayey sand; Massive grade of structure; Earthy fabric; Weak 
	consistence; 10-20%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 10-20%, medium 
	gravelly, 6-20mm, subangular, Quartz, coarse fragments; Field pH 6 (Raupach); Abrupt, Smooth change
	 to - 
	A12	0.05 - 0.35 m	Reddish brown (5YR4/4-Moist); ; Clayey coarse sand; Massive grade of structure; Earthy fabric; Weak 
	consistence; 10-20%, subrounded, Quartz, coarse fragments; 2-10%, subrounded, Granite, coarse 
	fragments; Field pH 6.5 (pH meter); 
	C	0.35 -  m	; 
	Morphological Notes
	C	Decomposing granite
	Observation Notes
	Site Notes

	Project Name:	Sandstone Yalgoo Paynes Find rangeland survey
	Project Code:	SYP	Site ID:	I016	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.5H	1B	0.52H	0.41	0.31	0.03	0.22J	1.27D
	0.05 - 0.1	5.9H	2B	1.63H	1.26	0.08	0.19	0.07J	3.16D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	120B	0.034E
	0.05 - 0.1	110B	0.034E
	Laboratory Analyses Completed for this profile
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour