Project Name:	Sandstone Yalgoo Paynes Find rangeland survey
	Project Code:	SYP	Site ID:	I023	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Peter Hennig	Locality:
	Date Desc.:	14/09/92	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6932265 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	734793  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Rock platform	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hyperbasic Petroclcic Calcic Calcarosol Medium Gravelly Loamy 	Principal Profile Form:	Uc1.13
	Loamy Very shallow
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A	0 - 0.15 m	Yellowish red (5YR3/6-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; Very weak 
	consistence; 10-20%, fine gravelly, 2-6mm, angular, Calcrete, coarse fragments; 2-10%, medium 
	gravelly, 6-20mm, angular, Calcrete, coarse fragments; Common (10 - 20 %), Calcareous, Fine (0 - 2 
	mm), Soft segregations; Soil matrix is Very highly calcareous; Field pH 9.5 (Raupach); 
	Dk	 - 0.15 m	; 
	Morphological Notes
	Dk	Calcrete. LD added TG April 2012
	Observation Notes
	Site Notes

	Project Name:	Sandstone Yalgoo Paynes Find rangeland survey
	Project Code:	SYP	Site ID:	I023	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	8.7H	120B	5.44E	1.24	0.79	1.03	8J	8.5D	12.88
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	110B	0.038E
	Laboratory Analyses Completed for this profile
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour