Project Name:	Sandstone Yalgoo Paynes Find rangeland survey
	Project Code:	SYP	Site ID:	I111	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Peter Hennig	Locality:
	Date Desc.:	28/10/92	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6844239 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	448426  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	15 % 	Aspect:	No Data
	Surface Soil Condition 	Surface crust, Hardsetting
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Paralithic Leptic Rudosol  Moderately gravelly Loamy  Very shallow	Principal Profile Form:	Um5.51
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A	0 - 0.1 m	Dark yellowish brown (10YR4/6-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; 
	Very weak consistence; 20-50%, angular, Consolidated rock (unidentified), coarse fragments; Field pH 6 
	(Raupach); 
	C	0.1 -  m	; 
	Morphological Notes
	C	Decomposed dolerite and schist
	Observation Notes
	Site Notes
	Slope previously codes as 150.
	Project Name:	Sandstone Yalgoo Paynes Find rangeland survey
	Project Code:	SYP	Site ID:	I111	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01	6.7H	4B	1.92A	3.36	0.4	0.19	7J	5.87D	2.71
	0.01 - 0.05	7.7H	3B	4.28A	6.79	0.34	0.36	11J	11.77D	3.27
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01	170B	0.053E
	0.01 - 0.05	120B	0.026E
	Laboratory Analyses Completed for this profile
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour