Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1379	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Angela Stuart-Street	Locality:
	Date Desc.:	25/05/99	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6229577 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	588279  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	135 degrees
	Surface Soil Condition 	Loose
	Erosion	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mottled-Mesonatric Yellow Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	2-10%, medium gravelly, 6-20mm, subrounded, Ironstone; No surface coarse fragments
	Profile Morphology
	A1p	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Fine sand; Moderately moist; Loose consistence; 2-10%, fine 
	gravelly, 2-6mm, subrounded, Ironstone, coarse fragments; Water repellent; Clear, Wavy change to - 
	A21ec	0.1 - 0.4 m	Light yellowish brown (10YR6/4-Moist); ; Fine sand; Moist; Loose consistence; 10-20%, fine gravelly, 2-
	6mm, subrounded, Ironstone, coarse fragments; Abrupt, Smooth change to - 
	B21	0.4 - 0.6 m	Brownish yellow (10YR6/6-Moist); , 10YR68, 10-20% , 5-15mm, Faint; , 2.5YR36, 10-20% , 5-15mm, 
	Prominent; Medium clay; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak 
	consistence; Clear, Wavy change to - 
	B22	0.6 - 0.8 m	Light yellowish brown (2.5Y6/4-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; , 2.5YR36, 10-20% , 5-
	15mm, Prominent; Medium clay; Weak grade of structure, 2-5 mm, Subangular blocky; Moist; Weak 
	consistence; Clear, Smooth change to - 
	B23	0.8 - 1 m	Light brownish grey (2.5Y6/3-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; Heavy clay; Massive grade 
	of structure; Sandy (grains prominent) fabric; Moist; Firm consistence; Clear, Smooth change to - 
	B31	1 - 1.4 m	Light yellowish brown (2.5Y6/4-Moist); , 2.5Y66, 10-20% , 5-15mm, Faint; Heavy clay; Massive grade of 
	structure; Sandy (grains prominent) fabric; Moist; Firm consistence; Clear, Wavy change to - 
	B32	1.4 - 1.8 m	Light grey (2.5Y7/2-Moist); , 2.5Y68, 10-20% , 5-15mm, Distinct; , 5YR34, 10-20% , 5-15mm, Distinct; 
	Heavy clay; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Firm consistence; 
	Abrupt, Smooth change to - 
	B33	1.8 - 1.9 m	Pale yellow (2.5Y7/3-Moist); , 2.5Y66, 10-20% , 15-30mm, Distinct; , 5YR34, 10-20% , 15-30mm, 
	Distinct; Heavy clay; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Firm 
	consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	near to crest of low broad rise - located where site TBO 0849 done.

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1379	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.8B	7A	1.22H	0.29	0.07	0.06	0.05J	1.64D
	5.6A
	0.1 - 0.4	4.6B	2A	0.33H	0.05	0.02	0.04	0.06J	0.44D
	5.5A
	0.4 - 0.6	4.8B	11A	1.31H	3.92	0.09	1.23	0.18J	6.55D
	6.1A
	0.6 - 0.8	4.7B	11A	0.68H	4.82	0.08	1.74	0.22J	7.32D
	6.2A
	0.8 - 1	5.7B	18A	0.66A	7.1	0.22	3.12	11.1D
	6.9A
	1 - 1.4	6.8B	21A	0.74A	7.95	0.26	4.64	13.59D
	8.2A
	1.4 - 1.8	7B	23A	0.68E	7.59	0.26	6.6	18B	15.13D	36.67
	8.4A
	1.8 - 1.9	7.1B	36A	0.71E	8.47	0.27	9.61	21B	19.06D	45.76
	8.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.78A	2	1.5
	0.1 - 0.4	0.13A	1.1	1.5
	0.4 - 0.6	0.25A	1.1	36
	0.6 - 0.8	0.2A	1.2	32.5
	0.8 - 1	0.1A	1.7	39.3
	1 - 1.4	0.08A	2.5	47.5
	1.4 - 1.8	0.06A	4.3	55.4
	1.8 - 1.9	0.05A	9.6	61.9
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1379	Observation 	1
	Agency Name:	Agriculture Western Australia
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B_AL	Aluminium in 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9A_S14	Total element - P(%) method S14 CCWA
	9I1	Phosphate sorption index
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75a	20 to 75u particle size analysis, (arithmetic difference)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)