Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1382	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Angela Stuart-Street	Locality:
	Date Desc.:	25/05/99	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6225470 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	576132  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Rises
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	225 degrees
	Surface Soil Condition 	Loose
	Erosion	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypercalcic Mottled-Mesonatric Grey Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments; No surface coarse fragments
	Profile Morphology
	A1p	0 - 0.1 m	Dark greyish brown (2.5Y4/2-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; Loose consistence; Sharp, Smooth change to - 
	A21e	0.1 - 0.5 m	Light brownish grey (2.5Y6/2-Moist); ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Moderately moist; Loose consistence; Sharp, Tongued change to - 
	B21	0.5 - 0.55 m	Light brownish grey (2.5Y6/3-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; Sandy medium clay; 
	Moderate grade of structure, Columnar; Sandy (grains prominent) fabric; Moderately moist; Firm 
	consistence; Clear, Smooth change to - 
	B22	0.55 - 0.7 m	Light olive brown (2.5Y5/6-Moist); , 7.5YR68, 10-20% , 5-15mm, Faint; Sandy light clay; Moderate grade 
	of structure, Columnar; Sandy (grains prominent) fabric; Moderately moist; Weak consistence; Gradual, 
	Smooth change to - 
	B23	0.7 - 0.9 m	Light yellowish brown (2.5Y6/4-Moist); , 2.5Y68, 10-20% , 5-15mm, Faint; Sandy medium clay; Weak 
	grade of structure, Polyhedral; Sandy (grains prominent) fabric; Moderately moist; Weak consistence; 
	Clear, Wavy change to - 
	B31k	0.9 - 1.1 m	Light yellowish brown (2.5Y6/4-Moist); , 2.5Y66, 2-10% , 5-15mm, Faint; Sandy medium clay; Weak grade
	 of structure, Polyhedral; Sandy (grains prominent) fabric; Moderately moist; Weak consistence; Few (2 - 
	10 %), Calcareous, Very coarse (20 - 60 mm), Nodules; Clear, Tongued change to - 
	B32k	1.1 - 1.3 m	Light yellowish brown (2.5Y6/4-Moist); , 10YR58, 10-20% , 30-mm, Faint; Sandy clay loam; Massive 
	grade of structure; Sandy (grains prominent) fabric; Moderately moist; Very weak consistence; Few (2 - 
	10 %), Calcareous, Very coarse (20 - 60 mm), Nodules; Clear, Wavy change to - 
	B33k	1.3 - 1.6 m	Light yellowish brown (2.5Y6/4-Moist); , 10YR68, 10-20% , 5-15mm, Distinct; Sandy light clay; Weak 
	grade of structure, Polyhedral; Sandy (grains prominent) fabric; Moderately moist; Weak consistence; 
	Few (2 - 10 %), Calcareous, Very coarse (20 - 60 mm), Nodules; 
	Morphological Notes
	Observation Notes
	Site Notes
	Pit on broadly undulating plain. Clay domed. Calcium carbonate appearing from 90cm. Pit located where site TBO #0865 done.

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1382	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9B	6A	3.32H	0.32	0.06	0.03	0.06J	3.73D
	5.7A
	0.1 - 0.5	5.2B	3A	0.43H	0.06	0.03	0.05	0.02J	0.57D
	6A
	0.5 - 0.55	5.2B	18A	1.9H	3.92	0.19	2.05	0.03J	8.06D
	6.5A
	0.55 - 0.7	7B	34A	1.59E	6.95	0.55	4.03	16B	13.12D	25.19
	8.3A
	0.7 - 0.9	7.8B	61A	1.48E	7.99	0.56	4.97	16B	15D	31.06
	8.8A
	0.9 - 1.1	8.7B	110A	1.6E	8.98	0.63	6.22	18B	17.43D	34.56
	9.4A
	1.1 - 1.3	8.7B	75A	0.89E	5.02	0.4	3.49	10B	9.8D	34.90
	9.6A
	1.3 - 1.6	8.3B	150A	1.38E	7.49	1.4	6.05	18B	16.32D	33.61
	9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.14A	1.6	2.2
	0.1 - 0.5	0.08A	1.2	1.5
	0.5 - 0.55	0.31A	5.9	26.6
	0.55 - 0.7	0.17A	2.8	37
	0.7 - 0.9	0.08A	2.7	35.3
	0.9 - 1.1	3.1C	0.07A	2.9	37
	1.1 - 1.3	<2C	0.04A	1.8	19.3
	1.3 - 1.6	1.7C	0.06A	3.5	56
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1382	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B_AL	Aluminium in 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9A_S14	Total element - P(%) method S14 CCWA
	9I1	Phosphate sorption index
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75a	20 to 75u particle size analysis, (arithmetic difference)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)