Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0146	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Henry Smolinski	Locality:
	Date Desc.:	13/02/97	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6195328 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	494300  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Hypernatric Yellow Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A11	0 - 0.15 m	Very dark grey (10YR3/1-Moist); ; Clayey sand; Single grain grade of structure; Moist; Field pH 6 
	(Raupach); 
	A12	0.15 - 0.6 m	Yellowish brown (10YR5/4-Moist); ; Clayey sand; Single grain grade of structure; Moist; 2-10%, medium
	 gravelly, 6-20mm, rounded, Ironstone, coarse fragments; Field pH 8 (Raupach); 
	B2	0.6 - 0.9 m	Yellowish brown (10YR5/8-Moist); , 2.5Y74, 10-20% ; , 2.5YR48, 2-10% ; Sandy light clay; Strong grade 
	of structure, 2-5 mm, Angular blocky; Moist; Field pH 8 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	Sampled

	Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0146	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5B	300B	2.86H	4.62	0.23	3.22	0.36J	10.93D
	5.9H
	0 - 0.1	5B	300B	2.86H	4.62	0.23	3.22	0.36J	10.93D
	5.9H
	0 - 0.1	5B	300B	2.86H	4.62	0.23	3.22	0.36J	10.93D
	5.9H
	0.15 - 0.6	6.3B	66B	1.27A	2.63	0.3	1.51	5.71D
	7.2H
	0.15 - 0.6	6.3B	66B	1.27A	2.63	0.3	1.51	5.71D
	7.2H
	0.15 - 0.6	6.3B	66B	1.27A	2.63	0.3	1.51	5.71D
	7.2H
	0.6 - 0.9	6.8B	94B	1.14A	5.95	0.45	3.76	11.3D
	7.5H
	0.6 - 0.9	6.8B	94B	1.14A	5.95	0.45	3.76	11.3D
	7.5H
	0.6 - 0.9	6.8B	94B	1.14A	5.95	0.45	3.76	11.3D
	7.5H
	0.6 - 0.9	6.8B	94B	1.14A	5.95	0.45	3.76	11.3D
	7.5H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	2.94D	370B	0.212E	5.4	4.4
	0 - 0.1	2.94D	370B	0.212E	5.4	4.4
	0 - 0.1	2.94D	370B	0.212E	5.4	4.4
	0.15 - 0.6	0.64D	78B	0.031E	2.9	8
	0.15 - 0.6	0.64D	78B	0.031E	2.9	8
	0.15 - 0.6	0.64D	78B	0.031E	2.9	8
	0.6 - 0.9	0.21D	54B	0.022E	11.5	46.4
	0.6 - 0.9	0.21D	54B	0.022E	11.5	46.4
	0.6 - 0.9	0.21D	54B	0.022E	11.5	46.4
	0.6 - 0.9	0.21D	54B	0.022E	11.5	46.4
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts

	Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0146	Observation 	1
	Agency Name:	Agriculture Western Australia
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)