Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0699	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Angela Stuart-Street	Locality:
	Date Desc.:	10/11/98	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6223706 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	476038  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Plain
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	2 % 	Aspect:	135 degrees
	Surface Soil Condition 	Firm
	Erosion	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic-Sodic Kurosolic Salic Hydrosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy fine sand; Field pH 4.9 (pH meter); Abrupt change to 
	- 
	A21	0.1 - 0.5 m	Dark yellowish brown (10YR4/4-Moist); ; Loamy sand; Field pH 5 (pH meter); Abrupt change to - 
	B21	0.5 - 0.75 m	Dark grey (2.5Y4/1-Moist); , 10YR68, 20-50% , 0-5mm, Prominent; Fine sandy light clay; Field pH 4.5 
	(pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Site close to drainage line on a bluegum plantation.  EC. of drainage line 8300 mS/m. Sample collected for sodicty analysis.

	Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0699	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.5 - 0.75	4.1B	61B	1.16H	8.45	0.03	3.63	0.98J	13.27D
	4.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.5 - 0.75	56.5I	1.5	42
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded