Project Name:	Wellington Blackwood land resources survey
	Project Code:	WBW	Site ID:	0992	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Peter Tille	Locality:
	Date Desc.:	17/12/92	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6263564 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	403104  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Red Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.15 m	Dark reddish brown (5YR3/3-Moist); ; Fine sandy loam; Weak grade of structure, ; Sandy (grains 
	prominent) fabric; Moist; 2-10%, fine gravelly, 2-6mm, Ironstone, coarse fragments; Clear change to - 
	A3	0.15 - 0.35 m	Red (2.5YR4/6-Moist); ; Sandy loam; Weak grade of structure, ; Sandy (grains prominent) fabric; Moist; 
	50-90%, medium gravelly, 6-20mm, Ironstone, coarse fragments; 0-2%, Quartz, coarse fragments; 
	Gradual change to - 
	B1	0.35 - 0.65 m	Red (2.5YR4/6-Moist); ; Clayey coarse sand; Weak grade of structure, ; Moderate grade of structure; 
	Sandy (grains prominent) fabric; Moist; 50-90%, medium gravelly, 6-20mm, Ironstone, coarse fragments;
	 Gradual change to - 
	B21	0.65 - 0.95 m	Red (2.5YR4/8-Moist); , 7.5YR58, 20-50% ; Light clay; Moderate grade of structure; Smooth-ped fabric; 
	Moist; 20-50%, Ironstone, coarse fragments; Clear change to - 
	B22	0.95 - 1.1 m	Red (2.5YR4/8-Moist); , 20-50% ; Silty medium clay; , Prismatic; Rough-ped fabric; Moist; 
	C	1.1 - 1.3 m	Light red (2.5YR7/6-Moist); ; 
	Morphological Notes
	B22	MOTTLES - Orange,yellow,grey
	C	ROCK -
	Observation Notes
	Site Notes
	ROCK SHISTOSE MICA

	Project Name:	Wellington Blackwood land resources survey
	Project Code:	WBW	Site ID:	0992	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	5.1B	17B	6.88H	1.23	1.17	0.26	0.32J	9.54D
	5.8H
	0.15 - 0.35	5.1B	4B	2.34H	0.72	0.43	0.08	0.13J	3.57D
	6H
	0.35 - 0.65	5.4B	2B	1.55H	0.97	0.27	0.05	<0.02J	2.84D
	6.2H
	0.65 - 0.95	5.7B	4B	0.85H	1.61	0.18	0.15	<0.02J	2.79D
	6.3H
	0.95 - 1.1	5B	11B	0.41H	3.51	0.04	0.75	<0.02J	4.71D
	5.6H
	1.3 - 1.3	4B	7B	0.38H	12.21	<0.02	3.96	2.73J	16.56D
	5.6H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	5.55D	960B	0.378E	9.9	4.1
	0.15 - 0.35	0.85D	170B	0.057E	7.3	12.8
	0.35 - 0.65	0.44D	120B	0.03E	8.1	16.9
	0.65 - 0.95	0.22D	99B	0.018E	9.1	27.7
	0.95 - 1.1	0.17D	47B	0.013E	8.8	48.6
	1.3 - 1.3	0.1D	32B	0.009E	9.3	17.2
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)

	Project Name:	Wellington Blackwood land resources survey
	Project Code:	WBW	Site ID:	0992	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)