Project Name:	BOC
	Project Code:	BOC	Site ID:	P101	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	T.R. Poutsma	Locality:	2.5KM south along road 1806 from junction of raod 
	1806 and road 6101:
	Date Desc.:	18/09/51	Elevation:	No Data
	Map Ref.:	Sheet No. : 2135   1:100000	Rainfall:	0
	Northing/Long.:	116.381944444444	Runoff:	Rapid
	Easting/Lat.:	-31.1666666666667	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Peneplain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Ferric-Petroferric Bleached-Leptic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1cb	0 - 0.13 m	Grey (10YR5/1-Moist); ; Sand; Single grain grade of structure; Dry; Loose consistence; Diffuse 
	change to - 
	A2	0.2 - 0.74 m	Light grey (10YR7/1-Moist); ; Sand; Single grain grade of structure; Dry; Loose consistence; 
	Diffuse, Irregular change to - 
	A3	0.74 - 0.91 m	Light olive grey (5Y6/2-Moist); ; Sand; Single grain grade of structure; Dry; Loose consistence; 
	Clear, Irregular change to - 
	B1	0.91 - 1.29 m	Light grey (5Y7/2-Moist); ; Sand; 50-90%, medium gravelly, 6-20mm, Substrate material, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	91-129CM GV FERRUGINISED (LOOSE AND CEMENTED):                                                                          
	Site Notes
	AVON LD

	Project Name:	BOC
	Project Code:	BOC	Site ID:	P101	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.9A	 0.015A
	0.2 - 0.74	5.8A	 0.009A
	0.74 - 0.91	6A	 0.012A
	0.91 - 1.29	6.4A	 0.015A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13
	0.2 - 0.74
	0.74 - 0.91
	0.91 - 1.29
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.2 - 0.74
	0.74 - 0.91
	0.91 - 1.29

	Project Name:	BOC
	Project Code:	BOC	Site ID:	P101	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour