Project Name:	DAN
	Project Code:	DAN	Site ID:	P451	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	Melbourne CG.308 - upslope from P450:
	Date Desc.:	02/08/61	Elevation:	No Data
	Map Ref.:	Sheet No. : 2036   1:100000	Rainfall:	0
	Northing/Long.:	115.698611111111	Runoff:	No Data
	Easting/Lat.:	-30.7069444444445	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 0.3 m deep,Limestone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcareous Petroclcic Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark reddish brown (5YR3/3-Moist); ; Sandy loam; Single grain grade of structure; Very weak 
	consistence; 
	0.05 - 0.13 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy loam (Heavy); Weak grade of structure, 5-10 mm, 
	Subangular blocky; Very weak consistence; 
	0.13 - 0.2 m	Dark red (2.5YR3/6-Moist); ; Sandy loam (Heavy); Weak grade of structure, 5-10 mm, Subangular 
	blocky; Very weak consistence; 
	k	0.2 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Very weak consistence; 20-50%, Limestone, coarse fragments; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P451	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.2A	 0.027A	 7.3K	 0.7	 0.51	 0.13
	0.05 - 0.13	6.5A	 0.018A	 7.2K	 1.1	 0.39	 0.13
	0.13 - 0.2	6.6A	 0.018A
	0.2 - 0.3	8.4A	 0.101A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.79D	 0.03D	 0.128B	<1	 35D	 50	 3	 10
	0.05 - 0.13	 1.1D	 0.023D	 0.081B	<1	 33D	 55	 2	 10
	0.13 - 0.2	<1	 30D	 57	 2	 12
	0.2 - 0.3	 0.034D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.13
	0.13 - 0.2
	0.2 - 0.3

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P451	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance