Project Name:	DAN
	Project Code:	DAN	Site ID:	P461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	4.8KM north of Dandaragan/Moora Rd.: on Rd which 
	turns off Dandaragan/Moora Rd about 24.3KM west of
	 Moora:
	Date Desc.:	01/08/61	Elevation:	No Data
	Map Ref.:	Sheet No. : 2036   1:100000	Rainfall:	0
	Northing/Long.:	115.771111111111	Runoff:	No Data
	Easting/Lat.:	-30.5972222222222	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Sand plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Backplain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	No Available Class Siliceous Arenic Rudosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Heath shrub, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Yellowish brown (10YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.05 - 0.1 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	0.15 - 0.25 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.25 - 0.33 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.33 - 0.41 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.51 - 0.58 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.66 - 0.76 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.89 - 0.99 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	1.73 - 1.83 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	2.54 - 2.74 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 2-10%, coarse gravelly, 20-60mm, Quartz, coarse fragments; 
	3.05 - 3.17 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 2-10%, Substrate material, coarse fragments; 
	3.25 - 3.4 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 2-10%, Substrate material, coarse fragments; 

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	3.66 - 3.81 m	Reddish yellow (5YR6/6-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	20-50%, Substrate material, coarse fragments; 
	4.11 - 4.27 m	Reddish yellow (7.5YR6/8-Moist); , 2.5YR46; Sand; Single grain grade of structure; Very weak 
	consistence; 20-50%, Substrate material, coarse fragments; Very few (0 - 2 %), Unidentified, , 
	Concretions; 
	4.65 - 4.8 m	Reddish yellow (7.5YR6/8-Moist); , 2.5YR48; , 5YR66; Sand; Single grain grade of structure; 
	Very weak consistence; 20-50%, Substrate material, coarse fragments; Very few (0 - 2 %), 
	Unidentified, , Concretions; 
	Morphological Notes
	Observation Notes
	305-480CM AL GV IS FERRUGINOUS (LATERITE):305-340CM <10% <60MM QZ ALSO:>480CM STOPPED BY COARSE VERY
	 HARD LATERITE GV:  
	Site Notes

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A	 0.009A	 0.7K	 0.4	<0.01	 0.06
	0.05 - 0.1	6.5A	 0.009A	 0.8K	 0.4	<0.01	<0.01
	0.15 - 0.25	6.4A	 0.009A
	0.25 - 0.33	6.4A	 0.009A
	0.33 - 0.41	6.5A	 0.009A
	0.51 - 0.58	6.5A	 0.009A
	0.66 - 0.76	6.3A	 0.009A
	0.89 - 0.99	6.3A	 0.009A
	1.73 - 1.83	6.2A	 0.012A
	2.54 - 2.74	5.9A	 0.012A
	3.05 - 3.17	6.1A	 0.012A
	3.25 - 3.4	6.1A	 0.012A
	3.66 - 3.81	6.1A	 0.012A
	4.11 - 4.27	6A	 0.015A
	4.65 - 4.8	5.8A	 0.018A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.42D	 0.005D	 0.015B	 0.012C	<1	 45D	 49	 3	 2
	0.05 - 0.1	 0.37D	 0.002D	 0.015B	 0.012C	<1	 46D	 47	<1	 5
	0.15 - 0.25
	0.25 - 0.33	 0.002D	 0.012C	 1	 42D	 50	<1	 5
	0.33 - 0.41
	0.51 - 0.58	 0.003D	 0.012C	 1	 39D	 53	 2	 6
	0.66 - 0.76
	0.89 - 0.99	 0.003D	 0.012C	 1	 35D	 56	 2	 6
	1.73 - 1.83
	2.54 - 2.74	 0.003D	 0.008C	 6	 29D	 59	 2	 9
	3.05 - 3.17
	3.25 - 3.4	 0.003D	 0.012C	 60	 31D	 56	 2	 11
	3.66 - 3.81
	4.11 - 4.27	 0.002D	 0.008C	 47	 32D	 49	 3	 15
	4.65 - 4.8	 0.003D	 0.008C	 32	 28D	 48	 4	 19
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.15 - 0.25
	0.25 - 0.33
	0.33 - 0.41
	0.51 - 0.58
	0.66 - 0.76
	0.89 - 0.99
	1.73 - 1.83
	2.54 - 2.74
	3.05 - 3.17

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	3.25 - 3.4
	3.66 - 3.81
	4.11 - 4.27
	4.65 - 4.8

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P461	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_HCL	Total element - K(%) - By boiling HCl
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance