Project Name:	DAN
	Project Code:	DAN	Site ID:	P467	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	Near northern part of location M517 Melbourne:
	Date Desc.:	29/08/61	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Sand plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); , 5YR58, 2-10% ; , 2-10% ; Sand; Single grain grade of
	 structure; Very weak consistence; 
	0.05 - 0.13 m	Very dark greyish brown (10YR3/2-Moist); , 5YR58, 2-10% ; , 2-10% ; Sand; Single grain grade of
	 structure; Very weak consistence; 
	0.15 - 0.25 m	Brown (10YR4/3-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	0.33 - 0.41 m	Brown (7.5YR4/4-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	0.56 - 0.66 m	Brown (7.5YR4/4-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	0.74 - 0.81 m	Yellowish red (5YR4/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	0.96 - 1.07 m	Yellowish red (5YR4/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	1.68 - 1.83 m	Yellowish red (5YR5/6-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	1.98 - 2.13 m	Yellowish red (5YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	2.54 - 1.74 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	3.66 - 3.81 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	4.27 - 4.42 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	Morphological Notes
	Observation Notes
	0-13CM SOME ORANGE (5YR58) SAND PIPES:                                                                                  
	Site Notes

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P467	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.9A	 0.119A	 2.3K	 0.7	 0.09	 0.08
	0.05 - 0.13	6A	 0.036A	 1.7K	 0.5	 0.08	 0.1
	0.15 - 0.25	6.4A	 0.015A
	0.33 - 0.41	6.6A	 0.015A
	0.56 - 0.66	6.7A	 0.012A
	0.74 - 0.81	6.7A	 0.012A
	0.96 - 1.07	6.7A	 0.012A
	1.68 - 1.83	6.8A	 0.009A
	1.98 - 2.13	6.8A	 0.012A
	2.54 - 2.74	6.8A	 0.009A
	3.66 - 3.81	6.7A	 0.012A
	4.27 - 4.42	6.4A	 0.018A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.91D	 0.031D	 0.063B	 0.011C	<1	 54D	 42	 2	 2
	0.05 - 0.13	 0.68D	 0.032D	 0.038B	 0.016C	<1	 46D	 49	 1	 2
	0.15 - 0.25
	0.33 - 0.41	 0.023D	 0.01C	<1	 50D	 46	 3	 2
	0.56 - 0.66
	0.74 - 0.81	 0.028D	 0.014C	<1	 48D	 48	 3	 2
	0.96 - 1.07
	1.68 - 1.83	 0.016D	 0.01C	<1	 44D	 51	 1	 4
	1.98 - 2.13
	2.54 - 2.74	 0.011D	 0.01C	<1	 41D	 54	 1	 4
	3.66 - 3.81
	4.27 - 4.42	 0.008D	 0.01C	<1	 54D	 40	 1	 3
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.13
	0.15 - 0.25
	0.33 - 0.41
	0.56 - 0.66
	0.74 - 0.81
	0.96 - 1.07
	1.68 - 1.83
	1.98 - 2.13
	2.54 - 2.74
	3.66 - 3.81
	4.27 - 4.42

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P467	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_HCL	Total element - K(%) - By boiling HCl
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance