Project Name:	DAN
	Project Code:	DAN	Site ID:	P469	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	Northern part of M517 Melbourne:
	Date Desc.:	30/08/61	Elevation:	No Data
	Map Ref.:	Sheet No. : 2036   1:100000	Rainfall:	0
	Northing/Long.:	115.676111111111	Runoff:	No Data
	Easting/Lat.:	-30.5502777777778	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Sand plain
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); , 7.5YR68; Sand; Single grain grade of structure; Very 
	weak consistence; 
	0.05 - 0.13 m	Brown (10YR4/3-Moist); , 7.5YR68; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.2 - 0.28 m	Strong brown (7.5YR5/6-Moist); , 10YR32; Sand; Single grain grade of structure; Very weak 
	consistence; 
	0.38 - 0.48 m	Strong brown (7.5YR5/6-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	0.63 - 0.76 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	1.07 - 1.22 m	Strong brown (7.5YR5/8-Moist); ; Sand; Single grain grade of structure; Very weak consistence; 
	1.78 - 1.93 m	Reddish yellow (7.5YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	2.49 - 2.69 m	Brownish yellow (10YR6/6-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	3.56 - 3.66 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P469	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.1A	 0.054A	 2.4K	 0.6	 0.1	 0.12
	0.05 - 0.13	5.9A	 0.018A	 1.3K	 0.5	 0.06	 0.02
	0.2 - 0.28	6.2A	 0.012A
	0.38 - 0.48	6.4A	 0.009A
	0.63 - 0.76	6.6A	 0.009A
	1.07 - 1.22	6.7A	 0.009A
	1.78 - 1.93	6.7A	 0.009A
	2.49 - 2.69	6.6A	 0.012A
	3.56 - 3.66	6.8A	 0.015A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.9D	 0.008D	 0.05B	 0.015C	<1	 48D	 46	 1	 5
	0.05 - 0.13	 0.62D	 0.006D	 0.036B	 0.015C	<1	 58D	 37	 2	 2
	0.2 - 0.28
	0.38 - 0.48	 0.004D	 0.01C	<1	 63D	 33	<1	 2
	0.63 - 0.76
	1.07 - 1.22	 0.004D	 0.012C	<1	 60D	 37	<1	 2
	1.78 - 1.93
	2.49 - 2.69	 0.003D	 0.01C	<1	 54D	 42	 2	 3
	3.56 - 3.66
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.13
	0.2 - 0.28
	0.38 - 0.48
	0.63 - 0.76
	1.07 - 1.22
	1.78 - 1.93
	2.49 - 2.69
	3.56 - 3.66

	Project Name:	DAN
	Project Code:	DAN	Site ID:	P469	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_HCL	Total element - K(%) - By boiling HCl
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance