Project Name:	DEN
	Project Code:	DEN	Site ID:	P2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	L.W. Pym	Locality:	Denmark - Mt.Barker Road 10.7KM south of location 
	52:
	Date Desc.:	01/04/49	Elevation:	No Data
	Map Ref.:	Sheet No. : 2328   1:100000	Rainfall:	No Data
	Northing/Long.:	117.430277777778	Runoff:	Rapid
	Easting/Lat.:	-34.8277777777778	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.06 m	Greyish brown (10YR5/2-Moist); ; Loamy sand; 50-90%, Substrate material, coarse fragments; 
	Clear change to - 
	0.06 - 0.3 m	Light yellowish brown (10YR6/4-Moist); ; Loamy sand (Heavy); 50-90%, Substrate material, 
	coarse fragments; Diffuse change to - 
	0.3 - 0.46 m	Light brown (7.5YR6/4-Moist); ; Sandy loam; 50-90%, Substrate material, coarse fragments; 
	Diffuse change to - 
	0.53 - 0.86 m	Brown (10YR4/3-Moist); , 10YR56; Medium clay; 10-20%, Substrate material, coarse fragments; 
	Diffuse change to - 
	Morphological Notes
	Observation Notes
	FERRUGINISED GRAVELS THROUGHOUT:86-140CM KAOLINITC TEX. CLAY WITH FE CONCRETIONS:                                
	       
	Site Notes
	HAY L.D.452/80

	Project Name:	DEN
	Project Code:	DEN	Site ID:	P2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.2A	 0.119A	 7.6K	 4	 0.36	 0.32	 12.5E	 24.8B
	0.06 - 0.3	6.3A	 0.051A	 2.5K	 1.8	 0.17	 0.14	 4.5E	 9.1B
	0.3 - 0.46	6.5A	 0.03A
	0.53 - 0.86	6.5A	 0.06A	 2.3K	 3.5	 0.29	 0.1	 5.2E	 11.4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 5.38D	 6D	 0.154B	 73	 25D	 47	 7	 14
	0.06 - 0.3	 1.5D	 4D	 0.051B	 68	 26D	 55	 7	 10
	0.3 - 0.46	 0.72D	 0.028B	 69	 31D	 49	 7	 11
	0.53 - 0.86	 0.62D	 5D	 0.025B	 25	 5D	 10	 8	 75
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.3
	0.3 - 0.46
	0.53 - 0.86

	Project Name:	DEN
	Project Code:	DEN	Site ID:	P2	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance