Project Name:	IRI
	Project Code:	IRI	Site ID:	P70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	Smith, R	Locality:	Avon location No.527:south side of road:
	Date Desc.:	08/02/51	Elevation:	 244 metres
	Map Ref.:	Rainfall:	430
	Northing/Long.:	Runoff:	Rapid
	Easting/Lat.:	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Grey Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	AB	0 - 0.1 m	Dark grey (10YR4/1-Moist); ; Clay loam; , Columnar; Weak consistence; 10-20%, Quartz, coarse 
	fragments; Diffuse change to - 
	B	0.15 - 0.38 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Massive grade of structure; Very firm consistence; 
	BC	0.38 - 0.61 m	Greyish brown (10YR5/2-Moist); ; Heavy clay; Very firm consistence; 2-10%, Substrate material, 
	coarse fragments; Diffuse change to - 
	C	0.69 - 0.91 m	Greyish brown (10YR5/2-Moist); , 10YR56; , 5Y52; Medium clay; 10-20%, Substrate material, 
	coarse fragments; 
	Morphological Notes
	Observation Notes
	38-91CM GV=W'D ROCK:                                                                                                    
	Site Notes

	Project Name:	IRI
	Project Code:	IRI	Site ID:	P70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.5A	 0.063A	 6.4K	 4	 0.2	 0.35	 11B
	0.15 - 0.38	7.2A	 0.095A	 11.5K	 11	 0.22	 2.34	 25.1B
	0.38 - 0.61	8.2A	 0.226A
	0.69 - 0.91	8.2A	 0.485A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.56D	 0.019D	 0.099B	 18	 44D	 29	 14	 14
	0.15 - 0.38	 0.82D	 0.02D	 0.08B	 18	 18D	 18	 8	 56
	0.38 - 0.61
	0.69 - 0.91
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.15 - 0.38
	0.38 - 0.61
	0.69 - 0.91

	Project Name:	IRI
	Project Code:	IRI	Site ID:	P70	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance